;*****************************************************************************
;*
;*  L1C62x86.INF  -   Qualcomm Atheros AR813X/AR815X/816X Series PCI-E Ethernet Controller
;*  Copyright 2004-, Atheros Co., Ltd.
;*
;*  Created on 01/04/2008 by Yu Hao
;*  INF File for NDIS6.2 Miniport Driver for Windows7 x86 
;*
;*****************************************************************************
[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHR%
CatalogFile = L1C62x86.cat
DriverVer   = 09/21/2012,2.1.0.12

[Manufacturer]
%ATHR% = Atheros, NTx86

[ControlFlags]

ExcludeFromSelect	= *


[Atheros.NTx86]
; DisplayName           Section                DeviceID
; -----------           -------	               --------
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063                                ; L1C
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_10631969&REV_C0

%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_83041043&REV_C0         ; ASUS
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_83FE1043&REV_C0         ; ASUS
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_84921043&REV_C0         ; ASUS
%ATHR.L1C%   =          L1C.DisS5.ndi,         PCI\VEN_1969&DEV_1063&SUBSYS_18201043&REV_C0         ; ASUS
%ATHR.L1C%   =          L1C.DisS5.ndi,         PCI\VEN_1969&DEV_1063&SUBSYS_18301043&REV_C0         ; ASUS

%ATHR.L1C%   =          L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_20081854&REV_C0         ; Pegatron
%ATHR.L1C%   =          L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_20091854&REV_C0         ; Pegatron
%ATHR.L1C%   =          L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_FF101854&REV_C0         ; Pegatron
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_202F1B0A&REV_C0         ; Pegatron
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_00C31B0A&REV_C0         ; Pegatron
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_00C91B0A&REV_C0         ; Pegatron

%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_10D217C0&REV_C0         ; M10B1
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_10D717C0&REV_C0         ; Dagger

%ATHR.L1C%   =          L1C.Lenovo.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_394E17AA&REV_C0         ; NAUR2,NAWA
%ATHR.L1C%   =          L1C.Lenovo.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_395817AA&REV_C0         ; NIMUA/B
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_395617AA&REV_C0         ; LU16_INTEL
%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_396117AA&REV_C0         ; LU16_AMD

%ATHR.L1C%   =          L1C.GIGABYTE.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_E0001458&REV_C0         ; GIGABYTE

%ATHR.L1C%   =          L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_81311019&REV_C0         ; ECS

%ATHR.L1C%   =       	L1C.Toshiba.ndi,       PCI\VEN_1969&DEV_1063&SUBSYS_FF501179&REV_C0         ; TZ2
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02291025&REV_C0         ; JM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_027F1025&REV_C0         ; JM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02801025&REV_C0         ; JM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02381025&REV_C0         ; SJM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02811025&REV_C0         ; SJM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02821025&REV_C0         ; SJM31
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_03021025&REV_C0         ; SJM52
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_03031025&REV_C0         ; SJM52
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_03041025&REV_C0         ; SJM52
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_022A1025&REV_C0         ; JM41
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_022B1025&REV_C0         ; JM51
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_034B1025&REV_C0         ; NCL20
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04301025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04311025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04321025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04331025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04341025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04111025&REV_C0         ; NCWH1
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041C1025&REV_C0         ; SJM30
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041D1025&REV_C0         ; SJM30
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_042B1025&REV_C0         ; SJM50
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_042C1025&REV_C0         ; SJM30
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04201025&REV_C0         ; SJM50NP_UMA
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04211025&REV_C0         ; SJM50NP_UMA
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041E1025&REV_C0         ; SJM50CP_UMA
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041F1025&REV_C0         ; SJM50CP_DIS
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_04501025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_044F1025&REV_C0         ; SJM40
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_049B1025&REV_C0         ; HM55_MV
                                                                                           
%ATHR.L1C%   =       	L1C.SONY.ndi,          PCI\VEN_1969&DEV_1063&SUBSYS_390217AA&REV_C0         ; LU15
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_395617AA&REV_C0         ; LA46
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_01671025&REV_C0         ; KAL90
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_021B1025&REV_C0         ; KBLG0
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02601025&REV_C0         ; KALG0
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_027D1025&REV_C0         ; NBLG0
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_01281025&REV_C0         ; KALH0
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_004214C0&REV_C0         ; NBLB1
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_004314C0&REV_C0         ; NBLB2
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_004514C0&REV_C0         ; NTTB1
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_004614C0&REV_C0         ; NTUC0
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_021E1025&REV_C0         ; ZK6
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_02531025&REV_C0         ; ZR6
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_026A1025&REV_C0         ; ZK8
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_026D1025&REV_C0         ; ZK8
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_026E1025&REV_C0         ; ZK8
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_029B1025&REV_C0         ; ZH7
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_029F1025&REV_C0         ; ZH8
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_029E1025&REV_C0         ; ZH6
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_03001025&REV_C0         ; ZE8
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_029D1025&REV_C0         ; ZE9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_03321025&REV_C0         ; ZH9
                                                                                           
%ATHR.L1C%   =       	L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_7009103C&REV_C0         ; SP7
%ATHR.L1C%   =       	L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_1522103C&REV_C0         ; Nikita
%ATHR.L1C%   =       	L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_147D103C&REV_C0         ; Nikita1.2
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1411103C&REV_C0         ; ZENO
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1412103C&REV_C0         ; ZENO
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1413103C&REV_C0         ; ZENO
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_142C103C&REV_C0         ; PETEK
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_142D103C&REV_C0         ; PETEK
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1421103C&REV_C0         ; Hamilton
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1423103C&REV_C0         ; Hamilton
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_1420103C&REV_C0         ; Prano
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_142B103C&REV_C0         ; Prano
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0D4E105B&REV_C0         ; AJ-BOX
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0D52105B&REV_C0         ; AJ-BOX-N
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0CD9105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0D56105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0CDA105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0E35105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0D57105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0CFC105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0CFD105B&REV_C0         ; Clone
%ATHR.L1C%   =       	L1C.ShutOn.ndi,        PCI\VEN_1969&DEV_1063&SUBSYS_0DC5105B&REV_C0         ; Clone
                                                                                           
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_07991854&REV_C0         ; QL2
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08001854&REV_C0         ; QL2
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08031854&REV_C0         ; QL4
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08041854&REV_C0         ; QL4
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08051854&REV_C0         ; QL2
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08071854&REV_C0         ; QL4
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08211854&REV_C0         ; QL4
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_08321854&REV_C0         ; QL4
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_20101854&REV_C0         ; PEGATRON
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_20111854&REV_C0         ; PEGATRON
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0809152D&REV_C0         ; SW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0810152D&REV_C0         ; SW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0812152D&REV_C0         ; TW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0813152D&REV_C0         ; TW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0814152D&REV_C0         ; SW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0815152D&REV_C0         ; TW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0822152D&REV_C0         ; TW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0828152D&REV_C0         ; TW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0831152D&REV_C0         ; TW9A
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0835152D&REV_C0         ; SW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0852152D&REV_C0         ; TW9D
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0853152D&REV_C0         ; TW9D
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0854152D&REV_C0         ; TW9E
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0855152D&REV_C0         ; SW9
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_0856152D&REV_C0         ; SW9D
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041E1028&REV_C0         ; Dell-DC1
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_041F1028&REV_C0         ; Dell-DC2
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_906A104D&REV_C0         ; NEO
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_9069104D&REV_C0         ; NEO
%ATHR.L1C%   =       	L1C.SONY.ndi,          PCI\VEN_1969&DEV_1063&SUBSYS_906F104D&REV_C0         ; Sony
%ATHR.L1C%   =       	L1C.SONY.ndi,          PCI\VEN_1969&DEV_1063&SUBSYS_9076104D&REV_C0         ; Cadiz
%ATHR.L1C%   =       	L1C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1063&SUBSYS_906C104D&REV_C0         ; TW6
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_907C104D&REV_C0         ; Tucana
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_9082104D&REV_C0         ; Tucana-BR
                                                                                           
%ATHR.L1C%   =       	L1C.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_10D217C0&REV_C0         ; M10B1
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062                                ; L2C
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_10621969&REV_C0         ; 
                                                                                           
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_83041043&REV_C0         ; ASUS
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_83FF1043&REV_C0         ; ASUS
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_838A1043&REV_C0         ; EEEPC
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_83BE1043&REV_C0         ; EEEPC
%ATHR.L2C%   =          L2C.DisS5.ndi,         PCI\VEN_1969&DEV_1062&SUBSYS_14E51043&REV_C0         ; F50Q
%ATHR.L2C%   =          L2C.DisS5.ndi,         PCI\VEN_1969&DEV_1062&SUBSYS_15251043&REV_C0         ; ASUS
                                                                                           
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_81321019&REV_C0         ; ECS
                                                                                           
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_20261B0A&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_1598103C&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.WOLMagic.ndi,      PCI\VEN_1969&DEV_1062&SUBSYS_00AA1B0A&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_20081854&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_20091854&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_200A1854&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_200B1854&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_200D1854&REV_C0         ; PEGATRON, H00J
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_200E1854&REV_C0         ; PEGATRON
%ATHR.L2C%   =          L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_00E01B0A&REV_C0         ; PEGATRON
                                                                                           
%ATHR.L2C%   =          L2C.GIGABYTE.ndi,      PCI\VEN_1969&DEV_1062&SUBSYS_E0001458&REV_C0         ; GIGABYTE
                                                                                           
%ATHR.L2C%   =          L2C.Lenovo.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_394F17AA&REV_C0         ; NAUR2,NAWA
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_38A317AA&REV_C0         ; LA14
%ATHR.L2C%   =          L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_395617AA&REV_C0         ; LA46
%ATHR.L2C%   =          L2C.Lenovo.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_395817AA&REV_C0         ; NIMUA/B
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_019C1025&REV_C0         ; KAV10
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02101025&REV_C0         ; KAWH0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02111025&REV_C0         ; KBWH0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02121025&REV_C0         ; KAWF0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02131025&REV_C0         ; KAWG0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02141025&REV_C0         ; HM40-MV
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02151025&REV_C0         ; HM40-YK
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02161025&REV_C0         ; HM20-YK
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_019D1025&REV_C0         ; 
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_022E1025&REV_C0         ; KAW10
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_022F1025&REV_C0         ; KAV50
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02301025&REV_C0         ; KAV60
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02411025&REV_C0         ; KAV80
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02431025&REV_C0         ; KAVA0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02601025&REV_C0         ; KALG0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_028D1025&REV_C0         ; HM50/70-PU
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_03491025&REV_C0         ; NAV50
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_034A1025&REV_C0         ; NAV60
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_030D1025&REV_C0         ; HM41
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_03501025&REV_C0         ; HM50/51/70
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04111025&REV_C0         ; NCWH1
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04391025&REV_C0         ; NAVD0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_043A1025&REV_C0         ; NAVD0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_043B1025&REV_C0         ; NAVE0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_043C1025&REV_C0         ; NAVE0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04591025&REV_C0         ; JE50_MV
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_045A1025&REV_C0         ; HM52_MV
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_045B1025&REV_C0         ; BA51_MV
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04971025&REV_C0         ; PAV50
                                                                                           
%ATHR.L2C%   =       	L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_308F103C&REV_C0         ; BIXBY
%ATHR.L2C%   =       	L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_1468103C&REV_C0         ; BIXBY 2.0
%ATHR.L2C%   =       	L2C.ShutOn.ndi,        PCI\VEN_1969&DEV_1062&SUBSYS_1492103C                ;  
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_0820152D&REV_C0         ; UW2
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04091028&REV_C0         ; ARGOS
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04431028&REV_C0         ; Phantom
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04511028&REV_C0         ; DJ
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04521028&REV_C0         ; DJ
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04531028&REV_C0         ; DJ
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04541028&REV_C0         ; DJ
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04651028&REV_C0         ; NAP10
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04661028&REV_C0         ; DJx
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04701028&REV_C0         ; NLM01
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04711028&REV_C0         ; NLM00
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_046F1028&REV_C0         ; DJ1_AMD
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04A61028&REV_C0	    ; DJ2_MV
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_049E1028&REV_C0	    ; DJ2_AMD
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_049F1028&REV_C0	    ; DJ2_CP_UMA
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_04A01028&REV_C0	    ; DJ2_CP_DIS
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_004414C0&REV_C0         ; NTTB0
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_004714C0&REV_C0         ; NTV00/10
                                                                                           
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_022C1025&REV_C0         ; ZG8
%ATHR.L2C%   =       	L2C.Toshiba.ndi,       PCI\VEN_1969&DEV_1062&SUBSYS_FF501179&REV_C0         ; TZ2
%ATHR.L2C%   =       	L2C.Toshiba.ndi,       PCI\VEN_1969&DEV_1062&SUBSYS_FFE01179&REV_C0         ; BU3
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_0790152D&REV_C0         ; IN1
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_02441025&REV_C0         ; ZA3
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_9064104D&REV_C0         ; SY2
%ATHR.L2C%   =       	L2C.ndi,               PCI\VEN_1969&DEV_1062&SUBSYS_9066104D&REV_C0         ; SY3
                                                                                           
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060			            ; L2cB        
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_20601969&REV_C1         ; L2cB
                                                                                             
%ATHR.L2CB%  =       	L2CB.PWMAll.ndi,       PCI\VEN_1969&DEV_2060&SUBSYS_FF1E1179&REV_C1         ; IEC
%ATHR.L2CB%  =       	L2CB.PWMAll.ndi,       PCI\VEN_1969&DEV_2060&SUBSYS_FDD01179&REV_C1         ; TE6

%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04511028&REV_C1         ; DJ1_MV                                                                                             
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04551028&REV_C1         ; UM7
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04561028&REV_C1         ; UM8
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04571028&REV_C1         ; UM9
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_04661028&REV_C1         ; DJ1_CP
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_046F1028&REV_C1         ; DJ1_AMD
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_04861028&REV_C1         ; DJ2_CP
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_04871028&REV_C1         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_048F1028&REV_C1         ; Dell_Avenger
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04901028&REV_C1         ; Dell_Voyager
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04A61028&REV_C1	    ; DJ2_MV
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_049E1028&REV_C1         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_049F1028&REV_C1         ; DJ2_CP_UMA
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04A01028&REV_C1         ; DJ2_CP_DIS
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04DF1028&REV_C1         ; Andros MLK
                                                                                             
%ATHR.L2CB%  =       	L2CB.ShutOn.ndi,       PCI\VEN_1969&DEV_2060&SUBSYS_147E103C&REV_C1         ; Bixby 3.0
                                                                                             
%ATHR.L2CB%  =       	L2CB.ShutOn.ndi,       PCI\VEN_1969&DEV_2060&SUBSYS_FD501179&REV_C1         ; TE2
%ATHR.L2CB%  =       	L2CB.ShutOn.ndi,       PCI\VEN_1969&DEV_2060&SUBSYS_FDD01179&REV_C1         ; BL6
                                                                                             
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_04291025&REV_C1         ; ZH9
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_043D1025&REV_C1         ; ZH9
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_043E1025&REV_C1         ; ZH9AB
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_03491025&REV_C1         ; NAV70
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_034A1025&REV_C1         ; NAV80
%ATHR.L2CB%  =       	L2CB.ASPM1.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_04971025&REV_C1         ; PAV50
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_048A1025&REV_C1         ; PEW72
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_05431025&REV_C1         ; P0VE6
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_05441025&REV_C1         ; P0VS6
                                                                                             
%ATHR.L2CB%  =       	L2CB.DisS5.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_396517AA&REV_C1         ; LL7
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_396B17AA&REV_C1         ; NAWEx
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_397917AA&REV_C1	    ; PIWG1/2/3
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_397B17AA&REV_C1	    ; PAWGx
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_398317AA&REV_C1	    ; PAW10/20
                                                                                             
%ATHR.L2CB%  =       	L2CB.MB.ndi,           PCI\VEN_1969&DEV_2060&SUBSYS_81521019&REV_C1         ; ECS
%ATHR.L2CB%  =       	L2CB.MB.ndi,           PCI\VEN_1969&DEV_2060&SUBSYS_20601019&REV_C1         ; ECS
                                                                                             
%ATHR.L2CB%  =       	L2CB.FUJU.ndi,         PCI\VEN_1969&DEV_2060&SUBSYS_15DB10CF&REV_C1         ; UME

%ATHR.L2CB%  =       	L2CB.DisS5.ndi,        PCI\VEN_1969&DEV_2060&SUBSYS_18501043&REV_C1         ; ASUS
%ATHR.L2CB%  =       	L2CB.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_84681043&REV_C1         ; ASUS

%ATHR.L2CB%  =       	L2CB.MB.ndi,           PCI\VEN_1969&DEV_2060&SUBSYS_E0001458&REV_C1         ; GIGABYTE
                                                                                             
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073			            ; L1d           
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_10731969&REV_C0         ; L1d
                                                                                             
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03561025&REV_C0         ; ZQ1
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03571025&REV_C0         ; ZQ1
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03581025&REV_C0         ; ZQ1B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03591025&REV_C0         ; ZQ1B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_035A1025&REV_C0         ; ZR7
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_035B1025&REV_C0         ; ZR7
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_035C1025&REV_C0         ; ZR7B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_035D1025&REV_C0         ; ZR7B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_035E1025&REV_C0         ; ZQ2
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03601025&REV_C0         ; ZR8
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03621025&REV_C0         ; ZR8B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03661025&REV_C0         ; ZQ2B
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03641025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03671025&REV_C0         ; ZYA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_03681025&REV_C0         ; ZYA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_038B1025&REV_C0         ; ZYB
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_038C1025&REV_C0         ; ZYB
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04121025&REV_C0         ; ZYD
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_040E1025&REV_C0         ; JV10
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04281025&REV_C0         ; SJV10
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04291025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_040D1025&REV_C0         ; SJV10_NL
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04601025&REV_C0         ; JV10_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_045F1025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04631025&REV_C0         ; ZR7D
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04641025&REV_C0         ; JV53_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04651025&REV_C0         ; JV53_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04731025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04751025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04761025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_047E1025&REV_C0         ; PAU30
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_048A1025&REV_C0         ; PEW72
%ATHR.L1D%  =       	L1D.TxPerf.ndi,	       PCI\VEN_1969&DEV_1073&SUBSYS_050E1025&REV_C0         ; P7YE0
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_050F1025&REV_C0         ; P7YE0
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_05131025&REV_C0         ; P7YS0
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_05141025&REV_C0         ; P7YS0
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_05151025&REV_C0         ; P7YH0
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_05161025&REV_C0         ; P7YH0
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_054C1025&REV_C0         ; JM30
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_054E1025&REV_C0         ; JM30
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_05221025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_05231025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_05241025&REV_C0         ; SJ53
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_052A1025&REV_C0         ; SJ53
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_05571025&REV_C0         ; JE41
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_055F1025&REV_C0         ; JE51
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_054B1025&REV_C0         ; HM51
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_054D1025&REV_C0         ; HM51
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_054F1025&REV_C0         ; JM40
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_055B1025&REV_C0         ; JM50
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_05711025&REV_C0         ; SJM40
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_056D1025&REV_C0         ; BA70
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_056F1025&REV_C0         ; SJM50
                                                                                             
%ATHR.L1D%  =       	L1D.ShutOn.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_FD501179&REV_C0         ; TE2
%ATHR.L1D%  =       	L1D.ShutOn.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_FDD01179&REV_C0         ; BL6
%ATHR.L1D%  =       	L1D.ToPatch.ndi,       PCI\VEN_1969&DEV_1073&SUBSYS_FF1E1179&REV_C0         ; Berlin
                                                                                             
%ATHR.L1D%  =       	L1D.DisS5.ndi,         PCI\VEN_1969&DEV_1073&SUBSYS_395B17AA&REV_C0         ; NAU00
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_396A17AA&REV_C0         ; NAWEx
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_395817AA&REV_C0         ; NIUM1
%ATHR.L1D%  =       	L1D.TxPerf.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_397917AA&REV_C0	    ; PIWG1/2/3
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_397B17AA&REV_C0	    ; PAWGx
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_398317AA&REV_C0	    ; PAW10/20
                                                                                             
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_0CDD105B&REV_C0         ; W930
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_0D5E105B&REV_C0         ; Haier
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_0DBE105B&REV_C0         ; Clone
                                                                                             
%ATHR.L1D%  =       	L1D.MB.ndi,            PCI\VEN_1969&DEV_1073&SUBSYS_81511019&REV_C0         ; ECS
%ATHR.L1D%  =       	L1D.MB.ndi,            PCI\VEN_1969&DEV_1073&SUBSYS_10731019&REV_C0         ; ECS
%ATHR.L1D%  =       	L1D.ECSD.ndi,          PCI\VEN_1969&DEV_1073&SUBSYS_04731028&REV_C0         ; ECS/Dell
                                                                                             
%ATHR.L1D%  =       	L1D.DisS5.ndi,         PCI\VEN_1969&DEV_1073&SUBSYS_18041043&REV_C0         ; ASUS
%ATHR.L1D%  =       	L1D.DisS5.ndi,         PCI\VEN_1969&DEV_1073&SUBSYS_18401043&REV_C0         ; ASUS

%ATHR.L1D%  =       	L1D.MB.ndi,            PCI\VEN_1969&DEV_1073&SUBSYS_E0001458&REV_C0         ; GIGABYTE

%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04511028&REV_C0         ; DJ1_MV
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04661028&REV_C0         ; DJ1_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_046F1028&REV_C0         ; DJ1_AMD
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04861028&REV_C0         ; DJ2_CP
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04871028&REV_C0         ; DJ2_AMD
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_048F1028&REV_C0         ; Dell_Avenger
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04901028&REV_C0         ; Dell_Voyager
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04A61028&REV_C0         ; DJ2_MV
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_049E1028&REV_C0         ; DJ2_AMD
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_049F1028&REV_C0         ; DJ2_CP_UMA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04A01028&REV_C0         ; DJ2_CP_DIS
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04911028&REV_C0         ; Spector
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04C81028&REV_C0         ; Alienware

%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_2AAE103C&REV_C0         ; Pegatron
%ATHR.L1D%  =       	L1D.ShutOn.ndi,        PCI\VEN_1969&DEV_1073&SUBSYS_207D1B0A&REV_C0         ; Pegatron

%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08611854&REV_C0	    ; QLH
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08621854&REV_C0	    ; QLH
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08631854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08641854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08651854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08661854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08671854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08681854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08691854&REV_C0         ; QLC
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08701854&REV_C0         ; QLC
%ATHR.L1D%  =       	L1D.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_08711854&REV_C0         ; QLC
                                                                                            
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062			            ; L2cb 2.0      
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_20621969&REV_C0
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04861028&REV_C0         ; DJ2_CP
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04871028&REV_C0         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04511028&REV_C0         ; DJ1_MV
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04551028&REV_C0         ; UM7
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04561028&REV_C0         ; UM8
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04571028&REV_C0         ; UM9
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04661028&REV_C0         ; DJ1_CP
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_046F1028&REV_C0         ; DJ1_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_048F1028&REV_C0         ; Dell_Avenger
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04901028&REV_C0         ; Dell_Voyager
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04A61028&REV_C0         ; DJ2_MV
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_049E1028&REV_C0         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_049F1028&REV_C0         ; DJ2_CP_UMA
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04A01028&REV_C0         ; DJ2_CP_DIS

%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD501179&REV_C0         ; TE2
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FDD01179&REV_C0         ; BL6
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FF1E1179&REV_C0         ; IEC
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_147E103C&REV_C0         ; Bixby 3.0                                                                                            
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C0         ; ZH9
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_043D1025&REV_C0         ; ZH9
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_043E1025&REV_C0         ; ZH9AB
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_03491025&REV_C0         ; NAV70
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_034A1025&REV_C0         ; NAV80
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04971025&REV_C0         ; PAV50
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_048A1025&REV_C0         ; PEW72
                                                                                             
%ATHR.L2CB%  =       	L2CB2.DisS5.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_396517AA&REV_C0         ; LL7
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_396B17AA&REV_C0         ; NAWEx
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_397917AA&REV_C0	    ; PIWG1/2/3
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_397B17AA&REV_C0	    ; PAWGx
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_398317AA&REV_C0	    ; PAW10/20
                                                                                             
%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_81521019&REV_C0         ; ECS
%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_20621019&REV_C0         ; ECS
                                                                                             
%ATHR.L2CB%  =       	L2CB2.FUJU.ndi,        PCI\VEN_1969&DEV_2062&SUBSYS_15DB10CF&REV_C0         ; UME

%ATHR.L2CB%  =       	L2CB2.DisS5.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_18501043&REV_C0         ; ASUS
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_84681043&REV_C0         ; ASUS

%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_E0001458&REV_C0         ; GIGABYT
      
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_20621969&REV_C1	    ; L2cb 2.1
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04861028&REV_C1         ; DJ2_CP
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04871028&REV_C1         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04511028&REV_C1         ; DJ1_MV
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04551028&REV_C1         ; UM7
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04561028&REV_C1         ; UM8
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04571028&REV_C1         ; UM9
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04661028&REV_C1         ; DJ1_CP
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_046F1028&REV_C1         ; DJ1_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_048F1028&REV_C1         ; Dell_Avenger
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04901028&REV_C1         ; Dell_Voyager
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04A61028&REV_C1         ; DJ2_MV
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_049E1028&REV_C1         ; DJ2_AMD
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_049F1028&REV_C1         ; DJ2_CP_UMA
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04A01028&REV_C1         ; DJ2_CP_DIS
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04DF1028&REV_C1         ; Andros MLK
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04EA1028&REV_C1         ; Zuma
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_051B1028&REV_C1         ; Shakira
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05501028&REV_C1         ; Avenger II
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05511028&REV_C1         ; Voyager II
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05521028&REV_C1         ; Spector II
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_057B1028&REV_C1         ; Voyager II
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05801028&REV_C1         ; Voyager II

%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC761179&REV_C1         ; Ankara
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC771179&REV_C1         ; Ankara
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD7A1179&REV_C1         ; Ankara
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD7B1179&REV_C1         ; Ankara
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC671179&REV_C1         ; Celtic
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD6A1179&REV_C1         ; Celtic
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD6B1179&REV_C1         ; Celtic
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD501179&REV_C1         ; TE2
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FDD01179&REV_C1         ; BL6
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FF1E1179&REV_C1         ; IEC
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FDD11179&REV_C1         ; TE7
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FFD61179&REV_C1         ; TZ6
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCB31179&REV_C1         ; TE7
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC501179&REV_C1         ; BLF
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCD01179&REV_C1         ; TE5
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCC01179&REV_C1         ; BU5
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD521179&REV_C1         ; BLE
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FDD21179&REV_C1         ; BU4
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FD401179&REV_C1         ; BU4
%ATHR.L2CB%  =       	L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC401179&REV_C1         ; BU6
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB901179&REV_C1         ; BU8
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB911179&REV_C1         ; BU8D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB921179&REV_C1         ; BU8D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCD31179&REV_C1         ; BY5/BY5D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB551179&REV_C1         ; BY6
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB561179&REV_C1         ; BY6D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCD21179&REV_C1         ; BY3
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCD41179&REV_C1         ; BY3D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCD51179&REV_C1         ; BY3D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC551179&REV_C1         ; BY4
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC561179&REV_C1         ; BY4D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC571179&REV_C1         ; BY4D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB501179&REV_C1         ; BY3C
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB511179&REV_C1         ; BY3G
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB521179&REV_C1         ; BY3G
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB801179&REV_C1         ; BY4C
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB811179&REV_C1         ; BY4G
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB821179&REV_C1         ; BY4G
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FCC51179&REV_C1         ; KZ1
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FC421179&REV_C1         ; BY1
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FBA01179&REV_C1         ; TEA
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FBA11179&REV_C1         ; BY2
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FBA21179&REV_C1         ; BY2D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FAB31179&REV_C1         ; BY2D
%ATHR.L2CB%  =          L2CB2.PWMAll.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_FB731179&REV_C1         ; BYD
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_147E103C&REV_C1         ; Bixby 3.0
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_3584103C&REV_C1         ; Kitty
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_3585103C&REV_C1         ; Kitty   
%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_3595103C&REV_C1         ; KID
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AE3103C&REV_C1         ; RedwoodA
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AE4103C&REV_C1         ; RedwoodB   
                                                                                             
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C1         ; ZH9
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_043D1025&REV_C1         ; ZH9
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_043E1025&REV_C1         ; ZH9AB
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_03491025&REV_C1         ; NAV70
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_034A1025&REV_C1         ; NAV80
%ATHR.L2CB%  =       	L2CB2.ASPM1.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_04971025&REV_C1         ; PAV50
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_048A1025&REV_C1         ; PEW72
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_02291025&REV_C1         ; JM31
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_027F1025&REV_C1         ; JM31
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_02801025&REV_C1         ; JM31
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_03641025&REV_C1         ; JM31
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_040E1025&REV_C1         ; JV10
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04281025&REV_C1         ; SJV10
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C1         ; JV10_NL
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_040D1025&REV_C1         ; SJV10_NL
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_04601025&REV_C1         ; SJV10_CP
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_045F1025&REV_C1         ; JV10_NL
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05431025&REV_C1         ; P0VE6
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05441025&REV_C1         ; P0VS6
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05981025&REV_C1         ; P1VE6
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06021025&REV_C1         ; HMA51-BZ
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06031025&REV_C1         ; ZQJ
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06041025&REV_C1         ; ZQQ
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_060A1025&REV_C1         ; SAZ70
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_060B1025&REV_C1         ; SIC70
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_060E1025&REV_C1         ; SAZ71
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_060F1025&REV_C1         ; SIC71
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06101025&REV_C1         ; AIC70
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06111025&REV_C1         ; AIC71
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06141025&REV_C1         ; AAB70
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06151025&REV_C1         ; AAB71
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_05041025&REV_C1         ;
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_061E1025&REV_C1         ; Q5WP1
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06221025&REV_C1         ; HMA41
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_06231025&REV_C1         ; HMA51
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_063A1025&REV_C1  	    ; JE10-CT
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_07641025&REV_C1  	    ; V5VE1/T1
                                                                                             
%ATHR.L2CB%  =       	L2CB2.DisS5.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_396517AA&REV_C1         ; LL7
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_396B17AA&REV_C1         ; NAWEx
%ATHR.L2CB%  =       	L2CB2.TxPerf.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_397917AA&REV_C1	    ; PIWG1/2/3
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_397B17AA&REV_C1	    ; PAWGx
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_397717AA&REV_C1	    ; Y490
                                                                                             
%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_81521019&REV_C1         ; ECS
%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_20621019&REV_C1         ; ECS
                                                                                             
%ATHR.L2CB%  =       	L2CB2.FUJU.ndi,        PCI\VEN_1969&DEV_2062&SUBSYS_15DB10CF&REV_C1         ; UME

%ATHR.L2CB%  =       	L2CB2.DisS5.ndi,       PCI\VEN_1969&DEV_2062&SUBSYS_18501043&REV_C1         ; ASUS
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_84681043&REV_C1         ; ASUS
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_100B1043&REV_C1         ; ASUS
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_103B1043&REV_C1  	    ; ASUS

%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_E0001458&REV_C1         ; GIGABYTE

%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_28021565&REV_C1         ; BIOSTAR
%ATHR.L2CB%  =       	L2CB2.MB.ndi,          PCI\VEN_1969&DEV_2062&SUBSYS_28011565&REV_C1         ; BIOSTAR

%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_207E1B0A&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AAE103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_3580103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AD1103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AD3103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AD4103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AE2103C&REV_C1         ; Pegatron
%ATHR.L2CB%  =       	L2CB2.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_2AF4103C&REV_C1         ; Pegatron

%ATHR.L2CB%  =       	L2CB2.ShutOn.ndi,      PCI\VEN_1969&DEV_2062&SUBSYS_0E2D105B&REV_C1         ; Livebox
%ATHR.L2CB%  =       	L2CB2.GIGABYTE.ndi,    PCI\VEN_1969&DEV_2062&SUBSYS_0D83105B&REV_C1         ; Foxconn

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083			            ; L1d 2.0          
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_10831969&REV_C0         ; 

%ATHR.L1D%  =       	L1D2.DisS5.ndi,        PCI\VEN_1969&DEV_1083&SUBSYS_18401043&REV_C0         ; ASUS
%ATHR.L1D%  =       	L1D2.DisS5.ndi,        PCI\VEN_1969&DEV_1083&SUBSYS_18511043&REV_C0         ; ASUS
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_847E1043&REV_C0         ; ASUS
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_84BF1043&REV_C0         ; ASUS
%ATHR.L1CD% =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_83FE1043&REV_C0         ; ASUS

%ATHR.L1D%  =       	L1D2.MB.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_E0001458&REV_C0         ; GIGABYTE

%ATHR.L1D%  =       	L1D2.MB.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_81511019&REV_C0         ; ECS
%ATHR.L1D%  =       	L1D2.MB.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_10831019&REV_C0         ; ECS

%ATHR.L1D%  =       	L1D2.MB.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_76801462&REV_C0         ; MSI

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_2AAE103C&REV_C0         ; Pegatron
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_3580103C&REV_C0         ; Pegatron
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_109C1462&REV_C0         ; Pegatron
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_208D1B0A&REV_C0         ; Pegatron
%ATHR.L1D%  =        	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_2AD5103C&REV_C0  	    ; Pegatron

%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3584103C&REV_C0         ; Kitty
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3585103C&REV_C0         ; Kitty
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3385103C&REV_C0         ; UMA
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3386103C&REV_C0         ; DIS
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1688103C&REV_C0         ; Lauren
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1689103C&REV_C0         ; Vuitton
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_168A103C&REV_C0         ; Vuitton

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04631025&REV_C0         ; ZR7D
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_047E1025&REV_C0         ; PAU30
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_048A1025&REV_C0         ; PEW72
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_050E1025&REV_C0         ; P7YE0
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_050F1025&REV_C0         ; P7YE0
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_05131025&REV_C0         ; P7YS0
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_05141025&REV_C0         ; P7YS0
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_05151025&REV_C0         ; P7YH0
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_05161025&REV_C0         ; P7YH0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_054C1025&REV_C0         ; JM30
%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_054E1025&REV_C0         ; JM30
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_02291025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_027F1025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_02801025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03641025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_040E1025&REV_C0         ; JV10
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04281025&REV_C0         ; SJV10
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04291025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_040D1025&REV_C0         ; SJV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04601025&REV_C0         ; SJV10_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_045F1025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03561025&REV_C0         ; ZQ1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03571025&REV_C0         ; ZQ1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03581025&REV_C0         ; ZQ1B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03591025&REV_C0         ; ZQ1B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_035A1025&REV_C0         ; ZR7
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_035B1025&REV_C0         ; ZR7
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_035C1025&REV_C0         ; ZR7B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_035D1025&REV_C0         ; ZR7B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_035E1025&REV_C0         ; ZQ2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03601025&REV_C0         ; ZR8
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03621025&REV_C0         ; ZR8B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03661025&REV_C0         ; ZQ2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03641025&REV_C0         ; JM31
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03671025&REV_C0         ; ZYA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_03681025&REV_C0         ; ZYA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_038B1025&REV_C0         ; ZYB
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_038C1025&REV_C0         ; ZYB
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04121025&REV_C0         ; ZYD
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_040E1025&REV_C0         ; JV10
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04281025&REV_C0         ; SJV10
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04291025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_040D1025&REV_C0         ; SJV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04601025&REV_C0         ; JV10_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_045F1025&REV_C0         ; JV10_NL
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04631025&REV_C0         ; ZR7D
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04641025&REV_C0         ; JV53_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04651025&REV_C0         ; JV53_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04731025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04751025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04761025&REV_C0         ; SJM70_CP
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_048A1025&REV_C0         ; PEW72
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_051E1025&REV_C0         ; SJV73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_051F1025&REV_C0         ; SJV73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05201025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05211025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05221025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05231025&REV_C0         ; JE73
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05241025&REV_C0         ; SJ53
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_052A1025&REV_C0         ; SJ53
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_052D1025&REV_C0         ; ZQE
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_052E1025&REV_C0         ; ZQE
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_052F1025&REV_C0         ; ZQG
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05301025&REV_C0         ; ZQG
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05571025&REV_C0         ; JE41
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_055F1025&REV_C0         ; JE51
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_054B1025&REV_C0         ; HM51
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_054D1025&REV_C0         ; HM51
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_054F1025&REV_C0         ; JM40
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_055B1025&REV_C0         ; JM50
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05711025&REV_C0         ; SJM40
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_056D1025&REV_C0         ; BA70
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_056F1025&REV_C0         ; SJM50
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05731025&REV_C0         ; ZRJ
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05741025&REV_C0         ; SJM40
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_058D1025&REV_C0         ; SJV51
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_058E1025&REV_C0         ; SJV51
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_059C1025&REV_C0         ; JE70
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_059D1025&REV_C0         ; SJV70
%ATHR.L1D%  =       	L1D2.PEGA.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_05391025&REV_C0         ; EIH30
%ATHR.L1D%  =       	L1D2.PEGA.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_053A1025&REV_C0         ; EIH31
%ATHR.L1D%  =       	L1D2.PEGA.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_060C1025&REV_C0         ; EIH30A
%ATHR.L1D%  =       	L1D2.PEGA.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_060D1025&REV_C0         ; EIH31A
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_064E1025&REV_C0  	    ; Q7YV0
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_064D1025&REV_C0  	    ; Q7YV0
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_064F1025&REV_C0  	    ; Q7YS0
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06501025&REV_C0  	    ; Q7YS0
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06511025&REV_C0  	    ; Q7YV1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06521025&REV_C0  	    ; Q7YV1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06531025&REV_C0  	    ; Q7YS1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06541025&REV_C0  	    ; Q7YS1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06631025&REV_C0  	    ; Q5WP3
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06741025&REV_C0  	    ; Q7YC1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06761025&REV_C0  	    ; Q7YC1
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06851025&REV_C0  	    ; VA70CR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06861025&REV_C0  	    ; VA70CR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06881025&REV_C0  	    ; VA70CR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06891025&REV_C0  	    ; VA70CR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_068A1025&REV_C0  	    ; VA70HR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_068B1025&REV_C0  	    ; VA70HR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_068C1025&REV_C0  	    ; VA70HR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_068D1025&REV_C0  	    ; VA70HR
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06961025&REV_C0  	    ; VA50_CM
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06981025&REV_C0  	    ; VG50_CM
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_06901025&REV_C0  	    ; Q5WT6
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05761025&REV_C0  	    ; BA50
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_07151025&REV_C0  	    ; ZQZ
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_07221025&REV_C0  	    ; BA50HC(CR)
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_07231025&REV_C0  	    ; BA50HC(HR)
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_073D1025&REV_C0  	    ; EG70_BZ
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_073E1025&REV_C0  	    ; EG70_BZ_PX
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_07561025&REV_C0  	    ; ZRP
%ATHR.L1D%  =        	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_07571025&REV_C0  	    ; ZRP

%ATHR.L1D%  =       	L1D2.WOLNone.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_048F1028&REV_C0         ; Dell_Avenger
%ATHR.L1D%  =       	L1D2.WOLNone.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_04901028&REV_C0         ; Dell_Voyager
%ATHR.L1D%  =       	L1D2.WOLNone.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_04911028&REV_C0         ; Spector
%ATHR.L1D%  =       	L1D2.WOLNone.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_04C81028&REV_C0         ; Alienware
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04A61028&REV_C0         ; DJ2_MV
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_049E1028&REV_C0         ; DJ2_AMD
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_049F1028&REV_C0         ; DJ2_CP_UMA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04A01028&REV_C0         ; DJ2_CP_DIS
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04371028&REV_C0         ; Miso
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04461028&REV_C0         ; Panerai
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_04841028&REV_C0         ; UMA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_051F1028&REV_C0         ; UMA1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05201028&REV_C0         ; UMA2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05211028&REV_C0         ; UMA3
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05221028&REV_C0         ; Discrete1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05231028&REV_C0         ; Discrete2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05241028&REV_C0         ; Discrete3
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05481028&REV_C0         ; Olympic
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_054B1028&REV_C0         ; Princeville
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05501028&REV_C0         ; Avenger II
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05511028&REV_C0         ; Voyager II
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05521028&REV_C0         ; Spector II
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_057B1028&REV_C0         ; Voyager II
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05801028&REV_C0         ; Voyager II

%ATHR.L1D%  =       	L1D2.TxPerf.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_397917AA&REV_C0	    ; PIWG1/2/3
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_397B17AA&REV_C0	    ; PAWGx
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_398317AA&REV_C0	    ; PAW10/20
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21EC17AA&REV_C0         ; Davis
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21ED17AA&REV_C0         ; Davis
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21EE17AA&REV_C0         ; Payton
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21EF17AA&REV_C0         ; Payton
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21F017AA&REV_C0         ; Payton
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21F117AA&REV_C0         ; Payton
%ATHR.L1D%  =       	L1D2.LVOn.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_21F217AA&REV_C0         ; Payton
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_397717AA&REV_C0	    ; Y490

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08611854&REV_C0	    ; QLH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08621854&REV_C0	    ; QLH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08631854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08641854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08651854&REV_C0         ; QLH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08661854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08671854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08681854&REV_C0         ; QLA
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08691854&REV_C0         ; QLC
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08701854&REV_C0         ; QLC
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08711854&REV_C0         ; QLC
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08891854&REV_C0         ; QLM
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08901854&REV_C0         ; QLM
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08911854&REV_C0         ; QLM
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08921854&REV_C0         ; QLM
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08961854&REV_C0         ; LG2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08971854&REV_C0         ; LG2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08981854&REV_C0         ; LG2
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_08991854&REV_C0         ; LG4
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09001854&REV_C0         ; LG4
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09011854&REV_C0         ; LG4
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09021854&REV_C0         ; LG7
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09031854&REV_C0         ; LG7
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09041854&REV_C0         ; LG7
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09061854&REV_C0         ; A430
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09071854&REV_C0         ; A430
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_09081854&REV_C0         ; A430
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_17911854&REV_C0         ; A420
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_17921854&REV_C0         ; A430
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_17931854&REV_C0         ; A430
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_17981854&REV_C0         ; LG2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_17991854&REV_C0         ; LG2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18001854&REV_C0         ; LG2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18011854&REV_C0         ; LG4B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18021854&REV_C0         ; LG4B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18031854&REV_C0         ; LG4B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18041854&REV_C0         ; LG2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18051854&REV_C0         ; LG2B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18061854&REV_C0         ; LG4B
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_18071854&REV_C0         ; LG4B

%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1650103C&REV_C0         ; Zidane UMA
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1651103C&REV_C0         ; Zidane SG
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3595103C&REV_C0         ; KID
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_3596103C&REV_C0         ; KID
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1851103C&REV_C0         ; Inventec / HP
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1852103C&REV_C0         ; Inventec / HP
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_1853103C&REV_C0         ; Inventec / HP

%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FDD11179&REV_C0         ; TE7
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FFD61179&REV_C0         ; TZ6
%ATHR.L1D%  =           L1D2.TOSHIBA.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_FF1E1179&REV_C0         ; WS2
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCB01179&REV_C0         ; TZ6
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC501179&REV_C0         ; BLF
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCD01179&REV_C0         ; TE5
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCC01179&REV_C0         ; BU5
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FD521179&REV_C0         ; BLE
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FDD21179&REV_C0         ; BU4
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FD401179&REV_C0         ; BU4
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FDD01179&REV_C0         ; TE4
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FD501179&REV_C0         ; BLG
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB901179&REV_C0         ; BU8
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB911179&REV_C0         ; BU8D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB921179&REV_C0         ; BU8D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCD31179&REV_C0         ; BY5/BY5D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB551179&REV_C0         ; BY6
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB561179&REV_C0         ; BY6D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCD21179&REV_C0         ; BY3
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCD41179&REV_C0         ; BY3D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCD51179&REV_C0         ; BY3D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC551179&REV_C0         ; BY4
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC561179&REV_C0         ; BY4D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC571179&REV_C0         ; BY4D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB501179&REV_C0         ; BY3C
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB511179&REV_C0         ; BY3G
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB521179&REV_C0         ; BY3G
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB801179&REV_C0         ; BY4C
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB811179&REV_C0         ; BY4G
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB821179&REV_C0         ; BY4G
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FCC51179&REV_C0         ; KZ1
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC421179&REV_C0         ; BY1
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FAB31179&REV_C0         ; BY2D
%ATHR.L1D%  =           L1D2.PWMAll.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FB721179&REV_C0         ; BYD
%ATHR.L1D%  =           L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_FC661179&REV_C0         ; Celtic

%ATHR.L1D%  =       	L1D2.SONY.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_9080104D&REV_C0         ; V050
%ATHR.L1D%  =       	L1D2.SONY.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_9081104D&REV_C0         ; V050
%ATHR.L1D%  =       	L1D2.WOLNone.ndi,      PCI\VEN_1969&DEV_1083&SUBSYS_908A104D&REV_C0         ; Z40/50
%ATHR.L1D%  =       	L1D2.SONY.ndi,         PCI\VEN_1969&DEV_1083&SUBSYS_908D104D&REV_C0         ; Z40/50BR

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0872152D&REV_C0         ; LG
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0873152D&REV_C0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0875152D&REV_C0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0876152D&REV_C0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0877152D&REV_C0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0878152D&REV_C0
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0883152D&REV_C0         ; SW6H
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0884152D&REV_C0         ; SW6H
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0880152D&REV_C0         ; SWH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0913152D&REV_C0         ; JW1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0914152D&REV_C0         ; JW1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0915152D&REV_C0         ; JW1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0916152D&REV_C0         ; JW1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0917152D&REV_C0         ; JW1
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0952152D&REV_C0         ; TWC
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0953152D&REV_C0         ; SWH
%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0988152D&REV_C0         ; JW8

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_10E717C0&REV_C0         ; M51

%ATHR.L1D%  =       	L1D2.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_0DBE105B&REV_C0         ; Clone
%ATHR.L1D%  =       	L1D2.ShutOn.ndi,       PCI\VEN_1969&DEV_1083&SUBSYS_0E2D105B&REV_C0         ; Livebox
%ATHR.L1D%  =       	L1D2.ECS.ndi,          PCI\VEN_1969&DEV_1083&SUBSYS_0D83105B&REV_C0         ; Foxconn	

%ATHR.L1D%  =       	L1D2.MB.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_28031565&REV_C0         ; BIOSTAR
			     	       
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091				    ; L1F

%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_85071043     	    ; ASUS
%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_200F1043     	    ; ASUS

%ATHR.L1F%  =        	L1F.MB.ndi,            PCI\VEN_1969&DEV_1091&SUBSYS_81611019     	    ; ECS

%ATHR.L1F%  =        	L1F.MB.ndi,            PCI\VEN_1969&DEV_1091&SUBSYS_E0001458     	    ; GIGABYTE

%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_AA5D1462	  	    ; MSI

%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_2AD5103C    	    ; Pegatron
%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_2AE0103C	    	    ; 

%ATHR.L1F%  =        	L1F.ShutOn.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_05001025	  	    ; JE40-CR
%ATHR.L1F%  =        	L1F.ShutOn.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_06431025	  	    ; JV42-HR

%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_397917AA	  	    ; Lenovo
%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_397817AA	  	    ;
%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_397C17AA	  	    ;
%ATHR.L1F%  =        	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_397717AA	  	    ; Y490

%ATHR.L1F%  =       	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_05481028	            ; Olympic
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_054B1028	            ; Princeville
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_055B1028	            ; M13
%ATHR.L1F%  =       	L1F.ShutOn.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_055C1028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_055D1028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_055E1028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_055F1028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05601028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05611028	            ; M13
%ATHR.L1F%  =       	L1F.ShutOn.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_05621028	            ; M13
%ATHR.L1F%  =       	L1F.ShutOn.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_05631028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05641028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05651028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05661028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05671028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05681028	            ; M13
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_057E1028                ; DMB40
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_057F1028                ; DMB40
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_058F1028                ; Z5_UMA
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_05901028                ; Z5_Discrete

%ATHR.L1F%  =       	L1F.ndi,      	       PCI\VEN_1969&DEV_1091&SUBSYS_17951854	            ; QLC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_17961854                ; QLC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_17971854         	    ; QLC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18081854         	    ; QLGA
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18091854	    	    ; LG3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18101854	    	    ; LG3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18111854	    	    ; LG3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18121854	    	    ; LG5
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18131854	    	    ; LG5
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18141854	    	    ; LG5
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18151854	    	    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18161854	    	    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18171854	    	    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18181854	    	    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18191854	    	    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18201854	    	    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18211854		    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18221854		    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18231854		    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18241854		    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18251854		    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18261854		    ; LG4C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18271854		    ; LG2C
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18281854		    ; LG4C

%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_20D61B0A	            ; Pegatron
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_20FA1B0A                ; Pegatron
%ATHR.L1F%  =       	L1F.PEGA.ndi,	       PCI\VEN_1969&DEV_1091&SUBSYS_01501B0A                ; Pegatron
%ATHR.L1F%  =       	L1F.PEGA.ndi,          PCI\VEN_1969&DEV_1091&SUBSYS_01571B0A                ; Pegatron

%ATHR.L1F%  =       	L1F.PWMALL.ndi,        PCI\VEN_1969&DEV_1091&SUBSYS_FF1E1179	            ; Toshiba

%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0925152D	            ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0926152D       	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0927152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0928152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0929152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0932152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0933152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0934152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0935152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0936152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0938152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0939152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0940152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0941152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0942152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0943152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0944152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0945152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0946152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0947152D         	    ; JW2
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0948152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0949152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0950152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0951152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0954152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0955152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0956152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0957152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0958152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0959152D         	    ; JW7
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0960152D         	    ; JW7
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0961152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0962152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0963152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0964152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0965152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0966152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0967152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0968152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0969152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0970152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0971152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0972152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0973152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0974152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0975152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0976152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0977152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0982152D         	    ; JW8
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0983152D         	    ; JW8
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0984152D         	    ; JW8
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0989152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0990152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0991152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0992152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0993152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0994152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0995152D         	    ; TWD
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_0997152D         	    ; JW6
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1001152D         	    ; TWC
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1006152D         	    ; JW6H
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1015152D         	    ; JW3
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1022152D         	    ; JW3H
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1030152D         	    ; JW9
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_1031152D         	    ; JW9

%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18291854         	    ; JW6L
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18301854         	    ; JW6L
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18311854         	    ; JW6L
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18321854         	    ; JW6L
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18331854         	    ; LG3B
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18341854         	    ; LG5B
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18351854         	    ; LG3B
%ATHR.L1F%  =       	L1F.ndi,               PCI\VEN_1969&DEV_1091&SUBSYS_18361854         	    ; LG5B

%ATHR.L1F%  =       	L1F.MB.ndi,            PCI\VEN_1969&DEV_1091&SUBSYS_00911969         	    ; iCafe

%ATHR.L1F%  =       	L1F.NEC.ndi,           PCI\VEN_1969&DEV_1091&SUBSYS_603317AA         	    ; NEC

%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090				    ; L2F

%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_397917AA	  	    ; Lenovo
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_397817AA	  	    ;
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_397C17AA    	    ;
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_397717AA    	    ; Y490

%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_055B1028	            ; M13
%ATHR.L2F%  =       	L2F.ShutOn.ndi,        PCI\VEN_1969&DEV_1090&SUBSYS_055C1028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_055D1028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_055E1028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_055F1028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05601028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05611028	            ; M13
%ATHR.L2F%  =       	L2F.ShutOn.ndi,        PCI\VEN_1969&DEV_1090&SUBSYS_05621028	            ; M13
%ATHR.L2F%  =       	L2F.ShutOn.ndi,        PCI\VEN_1969&DEV_1090&SUBSYS_05631028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05641028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05651028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05661028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05671028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05681028	            ; M13
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_058F1028	            ; Z5_UMA
%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_05901028	            ; Z5_Discrete

%ATHR.L2F%  =       	L2F.PWMALL.ndi,        PCI\VEN_1969&DEV_1090&SUBSYS_FF1E1179	            ; Toshiba

%ATHR.L2F%  =       	L2F.ndi,               PCI\VEN_1969&DEV_1090&SUBSYS_20FB1B0A                ; Pegatron

%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1                                ; L1H

%ATHR.L1H%  =       	L1F.MB.ndi,            PCI\VEN_1969&DEV_10A1&SUBSYS_00A11969         	    ; iCafe

%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_380017AA                ; VIQY0/Y1

%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_07671025                ; EA40_UMA
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_076B1025                ; EA50_UMA
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_076C1025                ; EA50_PowerXpress
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_076F1025                ; EG50_UMA
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_07701025                ; EG50_PowerXpress
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_07781025                ; VP40_UMA
%ATHR.L1H%  =       	L1F.ndi,               PCI\VEN_1969&DEV_10A1&SUBSYS_07791025                ; VP40_PowerXpress

%ATHR.L2H%  =           L2F.ndi,               PCI\VEN_1969&DEV_10A0				    ; L2H

%ATHR.L2H%  =       	L2F.ndi,               PCI\VEN_1969&DEV_10A0&SUBSYS_380017AA                ; VIQY0/Y1

[L1C.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.DisS5.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.Toshiba.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, Toshiba.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.Toshiba.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1C.Toshiba.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.Lenovo.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.Lenovo.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1C.Lenovo.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.SONY.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLNone.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.SONY.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.SONY.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1C.WOLMagic.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLMagic.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1C.WOLMagic.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1C.WOLMagic.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog
;-----------------------------------------------------------------------------

[L2C.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.Toshiba.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, Toshiba.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.Toshiba.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2C.Toshiba.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.Lenovo.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.Lenovo.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2C.Lenovo.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLMagic.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.SONY.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLNone.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.SONY.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.SONY.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.WOLMagic.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLMagic.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.WOLMagic.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.WOLMagic.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.FUJU.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, FUJU.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.FUJU.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.FUJU.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2C.ASPM1.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, ASPM1M.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2C.ASPM1.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2C.ASPM1.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, ShutOn.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.ECS.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, ShutOn.params, WOLMagic.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.ECS.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.ECS.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.MB.ndi]
Characteristics = 0x84
BusType         = 5	
DelReg          = Del.reg, EEELPI.Delreg			 ;PCI
AddReg          = L1C.reg, L2CB.params, MBCommon.params, ShutOn.params, WOLMagic.params, MSIIcafeLinkPatch.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.MB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.MB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.FUJU.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, FUJU.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.FUJU.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.FUJU.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB.ASPM1.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L2CB.params, Common.params, ShutOff.params, WOLDefault.params, ASPM1M.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB.ASPM1.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB.ASPM1.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2CB2.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.TxPerf.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.TxPerf.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.TxPerf.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.Toshiba.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, Toshiba.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.Toshiba.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2CB2.Toshiba.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.Lenovo.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.Lenovo.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2CB2.Lenovo.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.MB.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, MBCommon.params, ShutOn.params, WOLMagic.params, EEELPI.params, MSIIcafeLinkPatch.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.MB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.MB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.SONY.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLNone.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.SONY.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.SONY.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.WOLMagic.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.WOLMagic.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.WOLMagic.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L2CB2.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.FUJU.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, FUJU.params, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.FUJU.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.FUJU.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2CB2.ASPM1.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, ASPM1M.params, EEELPI.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2CB2.ASPM1.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2CB2.ASPM1.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.TxPerf.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.TxPerf.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.TxPerf.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.ToPatch.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params, ToPatch.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.ToPatch.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.ToPatch.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, WOLDefault.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, LongCable.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.MB.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, MB.params, ShutOn.params, WOLMagic.params, LongCable.params, ExRSS.params, MSIIcafeLinkPatch.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.MB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.MB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.ECS.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.ECS.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.ECS.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D.ECSD.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, ECS.params, ShutOn.params, WOLMagic.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D.ECSD.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D.ECSD.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, EEELPI.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D2.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.WOLNone.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLNone.params, EEELPI.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.WOLNone.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D2.WOLNone.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.TxPerf.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.TxPerf.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.TxPerf.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.LVOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, ECS.params, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params, Toshiba.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.LVOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.LVOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.LV.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, ECS.params, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.LV.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.LV.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D2.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, WOLDefault.params, EEELPI.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.DisS5.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, EEELPI.params, LongCable.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.MB.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, MB.params, ShutOn.params, WOLMagic.params, EEELPI.params, LongCable.params, ExRSS.params, MSIIcafeLinkPatch.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.MB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.MB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.ECS.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, EEELPI.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.ECS.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.ECS.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.SONY.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, WOLDefault.params, EEELPIEn.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.SONY.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D2.SONY.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.TOSHIBA.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.TOSHIBA.ndi.HW]
Include = machine.inf
Needs = PciASPMOptIn
Addreg = Msi.Addreg

[L1D2.TOSHIBA.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1D2.PEGA.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Pega.params, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params, ExRSS.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1D2.PEGA.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1D2.PEGA.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.PEGA.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, PEGAIP4.params, ShutOff.params, WOLDefault.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.PEGA.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.PEGA.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.GIGABYTE.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLMagic.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.GIGABYTE.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.GIGABYTE.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.MB.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, MB.params, ShutOn.params, WOLMagic.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params, MSIIcafeLinkPatch.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.MB.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.MB.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, Common.params, ShutOn.params, WOLDefault.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params, PWMAll.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L1F.NEC.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, L1C.params, FUJU.params, ShutOn.params, WOLNone.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1F.NEC.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.NEC.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2F.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOff.params, WOLDefault.params, PM.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2F.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L2F.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2F.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params, PM.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2F.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L2F.ShutOn.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog

[L2F.PWMAll.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
DelReg          = Del.reg, EEELPI.Delreg
AddReg          = L1C.reg, Common.params, ShutOn.params, WOLDefault.params, PM.params, EEELPI.params, Ecma.params, PWMAll.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2F.PWMAll.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L2F.PWMAll.ndi.Services]
AddService = L1C, 2, L1C.Service, L1C.EventLog
;-----------------------------------------------------------------------------
; L1C  specific
;
[L1C.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi, Service,    0, "L1C"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Msi.Addreg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[MsiX.Addreg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0

[Del.reg]
HKR, Ndi\Params\WakeUpCapabilities

[EEELPI.Delreg]
HKR, Ndi\Params\EEESupported

[L1C.Service]
DisplayName     = %L1C.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\L1C62x86.sys
LoadOrderGroup  = NDIS

[L1C.EventLog]
AddReg = L1C.AddEventLog.reg

[L1C.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\L1C62x86.sys"
HKR,, TypesSupported,	0x00010001, 7

[Toshiba.params]
HKR,, WOLMode,	        0x00010001, 1

[ToPatch.params]
HKR,, ToPatch,	        0x00010001, 1

[PWMNone.params]
HKR,, PnPCapabilities,	0x00010001, 0x0038

[PWM.params]
HKR,, PnPCapabilities,	0x00010001, 0x0020

[PWMAll.params]
HKR,, PnPCapabilities,	0x00010001, 0x0120

[ASPM1M.params]
HKR,, ASPMLim,	        0x00010001, 1

[ASPM10M.params]
HKR,, ASPMLim,	        0x00010001, 2

[ASPM100M.params]
HKR,, ASPMLim,	        0x00010001, 3

[LongCable.params]
HKR,, LongCable,        0x00010001, 1

[TxPerf.params]
HKR,, TxPerf,           0x00010001, 1

[Intr.params]
HKR,, MSIX,	        0x00010001, 1

[ASPMOff.params]
HKR,, L0SL1,            0x00010001, 0

[PHYHiberOff.params]
HKR,, PHYHiberOff,      0x00010001, 0

[MSIIcafeLinkPatch.params]
HKR,, MSIIcafeLinkPatch,0x00010001, 1

[L1C.params]
HKR, Ndi\Params\*JumboPacket,        		ParamDesc,  	0,      %JumboFrame%
HKR, Ndi\Params\*JumboPacket,        		default,    	0,      "1514"
HKR, Ndi\Params\*JumboPacket,        		type,       	0,      "enum"
HKR, Ndi\Params\*JumboPacket\enum,   		"1514",     	0,      %Disabled%
HKR, Ndi\Params\*JumboPacket\enum,   		"2048",     	0,      %2KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,   		"3072",     	0,      %3KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,   		"4096",     	0,      %4KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,   		"5120",     	0,      %5KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,   		"6144",     	0,      %6KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,   		"7168",     	0,      %7KBMTU%
HKR, Ndi\params\*JumboPacket\enum,   		"8192",     	0, 	%8KBMTU%
HKR, Ndi\params\*JumboPacket\enum,   		"9216",     	0, 	%9KBMTU%

[ExRSS.params]
HKR, Ndi\Params\RSS,				ParamDesc,	0,	%RSS%
HKR, Ndi\Params\RSS,				Type,		0,	"enum"
HKR, Ndi\Params\RSS\enum,			1,		0,	%Enabled%
HKR, Ndi\Params\RSS\enum,			0,		0,	%Disabled%
HKR, Ndi\Params\RSS,				Default,	0,	"0"

[RSS.params]
HKR, Ndi\Params\*RSS,				ParamDesc,	0,	%RSS%
HKR, Ndi\Params\*RSS,				Type,		0,	"enum"
HKR, Ndi\Params\*RSS\enum,			1,		0,	%Enabled%
HKR, Ndi\Params\*RSS\enum,			0,		0,	%Disabled%
HKR, Ndi\Params\*RSS,				Default,	0,	"1"

HKR, Ndi\Params\*NumRssQueues,			ParamDesc,	0,	%RssQs%
HKR, Ndi\Params\*NumRssQueues,			Type,		0,	"enum"
;HKR, Ndi\Params\*NumRssQueues\enum,		"8",		0,	"8 RSS Queues"
;HKR, Ndi\Params\*NumRssQueues\enum,		"6",		0,	"6 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,		"4",		0,	"4 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,		"2",		0,	"2 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,		"1",		0,	"1 RSS Queues"
HKR, Ndi\Params\*NumRssQueues,			Default,	0,	"4"

[L2CB.params]
HKR, Ndi\Params\APSmode,    	                ParamDesc,      0,      %APSmode%
HKR, Ndi\Params\APSmode,    	                Type,           0,      "enum"
HKR, Ndi\Params\APSmode\enum, 	                "1",            0,      %Enabled%
HKR, Ndi\Params\APSmode\enum, 	                "0",            0,      %Disabled%
HKR, Ndi\Params\APSmode,    	                Default,        0,      "0"
;-----------------------------------------------------------------------------

[Ecma.params]
HKR, Ndi\Params\Ecma,    	                ParamDesc,      0,      %ECMA%
HKR, Ndi\Params\Ecma,    	                Type,           0,      "enum"
HKR, Ndi\Params\Ecma\enum, 	                "1",            0,      %Enabled%
HKR, Ndi\Params\Ecma\enum, 	                "0",            0,      %Disabled%
HKR, Ndi\Params\Ecma,    	                Default,        0,      "0"

[Common.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"1"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "1"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "1"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"3"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[PEGAIP4.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"0"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "1"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"3"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[MBCommon.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"0"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"0"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"3"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[Pega.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "1024"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"1"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"3"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[FUJU.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"1"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"0"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[ECS.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"6",		0,	%1GFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"1"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"0"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[MB.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0,	%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0,	"int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0,	"10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0,	"1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0,	"30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0,	"500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0,	"5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0,	%SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0,	"enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0,	"0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0,	%Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0,	%10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0,	%10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0,	%100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0,	%100MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"6",		0,	%1GFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0,      "512"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0,      "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0,      "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0,      "16"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0,      "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, 	%TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, 	%IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, 	"enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, 	"0"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, 	%UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, 	"3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, 	%TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, 	%UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, 	"enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, 	%RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, 	%TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, 	"3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, 	%LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, 	"enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, 	"0"

HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,			Default,	0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,		"1",		0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,		"0",		0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,			Default,	0,      "0"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, 	%NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, 	"edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, 	"12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, 	"1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, 	""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, 	"1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, 	%IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, 	"enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, 	"1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, 	%FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, 	"enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, 	%TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, 	"3"

HKR, Ndi\Params\VLanID,				ParamDesc,	0,      %VLanID%
HKR, Ndi\Params\VLanID,				Type,		0,      "long"
HKR, Ndi\Params\VLanID,				Base,	        0,      "10"
HKR, Ndi\Params\VLanID,				Min,	        0,      "0"
HKR, Ndi\Params\VLanID,				Max,	        0,      "4094"
HKR, Ndi\Params\VLanID,				Step,	        0,      "1"
HKR, Ndi\Params\VLanID,				Default,	0,      "0"

[WOLDefault.params]
HKR, Ndi\Params\*WakeOnMagicPacket,		ParamDesc,	0, 	%MagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket,		Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,		Default,	0, 	"1"

HKR, Ndi\Params\*WakeOnPattern,			ParamDesc,	0, 	%PatternMatch%
HKR, Ndi\Params\*WakeOnPattern,			Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnPattern\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnPattern,			Default,	0, 	"1"

[WOLMagic.params]
HKR, Ndi\Params\*WakeOnMagicPacket,		ParamDesc,	0, 	%MagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket,		Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,		Default,	0, 	"1"

HKR, Ndi\Params\*WakeOnPattern,			ParamDesc,	0, 	%PatternMatch%
HKR, Ndi\Params\*WakeOnPattern,			Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnPattern\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnPattern,			Default,	0, 	"0"

[WOLNone.params]
HKR, Ndi\Params\*WakeOnMagicPacket,		ParamDesc,	0, 	%MagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket,		Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,		Default,	0, 	"0"

HKR, Ndi\Params\*WakeOnPattern,			ParamDesc,	0, 	%PatternMatch%
HKR, Ndi\Params\*WakeOnPattern,			Type,		0, 	"enum"
HKR, Ndi\Params\*WakeOnPattern\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*WakeOnPattern,			Default,	0, 	"0"

[PM.params]
HKR, Ndi\Params\*PMARPOffload,			ParamDesc,	0, 	%ARPOffload%
HKR, Ndi\Params\*PMARPOffload,			Type,		0, 	"enum"
HKR, Ndi\Params\*PMARPOffload\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*PMARPOffload\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*PMARPOffload,			Default,	0, 	"1"

HKR, Ndi\Params\*PMNSOffload,			ParamDesc,	0, 	%NSOffload%
HKR, Ndi\Params\*PMNSOffload,			Type,		0, 	"enum"
HKR, Ndi\Params\*PMNSOffload\enum,		"1",		0, 	%Enabled%
HKR, Ndi\Params\*PMNSOffload\enum,		"0",		0, 	%Disabled%
HKR, Ndi\Params\*PMNSOffload,			Default,	0, 	"1"

[ShutOn.params]
HKR, Ndi\Params\ShutdownWake,			ParamDesc,	0,	 %ShutDW%
HKR, Ndi\Params\ShutdownWake,			Type,		0,	 "enum"
HKR, Ndi\Params\ShutdownWake\enum,		1,		0,	 %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,		0,		0,	 %Disabled%
HKR, Ndi\Params\ShutdownWake,			Default,	0,	 "1"

[ShutOff.params]
HKR, Ndi\Params\ShutdownWake,			ParamDesc,	0,	 %ShutDW%
HKR, Ndi\Params\ShutdownWake,			Type,		0,	 "enum"
HKR, Ndi\Params\ShutdownWake\enum,		1,		0,	 %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,		0,		0,	 %Disabled%
HKR, Ndi\Params\ShutdownWake,			Default,	0,	 "0"

[EEELPI.params]
HKR, Ndi\Params\*EEE,    	                ParamDesc,      0,       %EEE%
HKR, Ndi\Params\*EEE,    	                Type,           0,       "enum"
HKR, Ndi\Params\*EEE\enum, 	                "1",            0,       %Enabled%
HKR, Ndi\Params\*EEE\enum, 	                "0",            0,       %Disabled%
HKR, Ndi\Params\*EEE,    	                Default,        0,       "0"

[EEELPIEn.params]
HKR, Ndi\Params\*EEE,    	                ParamDesc,      0,       %EEE%
HKR, Ndi\Params\*EEE,    	                Type,           0,       "enum"
HKR, Ndi\Params\*EEE\enum, 	                "1",            0,       %Enabled%
HKR, Ndi\Params\*EEE\enum, 	                "0",            0,       %Disabled%
HKR, Ndi\Params\*EEE,    	                Default,        0,       "1"
;-----------------------------------------------------------------------------
; DestinationDirs
;
[L1C.CopyFiles]
L1C62x86.sys,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DriverDisk%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
L1C62x86.sys = 1

[DestinationDirs]
L1C.CopyFiles     	= 12
DefaultDestDir       	= 11

[Strings]
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Interrupt Moderation"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max IRQ per Second"
Enabled			 = "Enabled"
Disabled		 = "Disabled"
SpeedDuplex		 = "Speed & Duplex"
Auto		  	 = "Auto Negotiation"
1GFD                     = "1.0 Gbps Full Duplex"
10MHD		  	 = "10 Mbps Half Duplex"
10MFD		  	 = "10 Mbps Full Duplex"
100MHD			 = "100 Mbps Half Duplex"
100MFD			 = "100 Mbps Full Duplex"
FlowCtrl		 = "Flow Control"
ShutDW			 = "Shutdown Wake Up"
RSS			 = "Receive Side Scaling"
TXEna 			 = "Tx Enabled"
RXEna 			 = "Rx Enabled"
TXRXEna 		 = "Rx & Tx Enabled"
ReceiveBuffers 		 = "Receive Buffers"
TransmitBuffers 	 = "Transmit Buffers"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
LSOv2IPv4 		 = "Large Send Offload v2 (IPv4)"
LSOv2IPv6 		 = "Large Send Offload v2 (IPv6)"
NetAddress   		 = "Network Address"
WakeUpCapabilities       = "Wake Up Capabilities"
APSmode			 = "APS mode"
AZPower                  = "802.3az"
None		         = "None"
LinkChange	         = "Link Change"
MagicPacket	         = "Wake on magic packet"
PatternMatch	         = "Wake on pattern match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "All"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "Maximum Number of RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Chinese (Taiwan)
[Strings.0404]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "大型框架"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "中斷調節"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "每秒 IRQ 上限"
Enabled			 = "已啟用"
Disabled		 = "已停用"
SpeedDuplex		 = "速度和雙工"
Auto		  	 = "自動協調"
1GFD                     = "1.0 Gbps 全雙工"
10MHD		  	 = "10 Mbps 半雙工"
10MFD		  	 = "10 Mbps 全雙工"
100MHD			 = "100 Mbps 半雙工"
100MFD			 = "100 Mbps 全雙工"
FlowCtrl		 = "FlowControl"
ShutDW			 = "關閉狀態喚醒"
RSS			 = "接收側邊調整"
TXEna 			 = "傳輸已啟用"
RXEna 			 = "接收已啟用"
TXRXEna 		 = "傳輸和接收已啟用"
ReceiveBuffers 		 = "接收緩衝"
TransmitBuffers 	 = "傳輸緩衝"
IPChksumOffv4 		 = "IPv4 檢查總和卸載"
TCPChksumOffv4 		 = "TCP 檢查總和卸載 (IPv4)"
TCPChksumOffv6 		 = "TCP 檢查總和卸載 (IPv6)"
UDPChksumOffv4 		 = "UDP 檢查總和卸載 (IPv4)"
UDPChksumOffv6 		 = "UDP 檢查總和卸載 (IPv6)"
LSOv1IPv4 		 = "大型傳送卸載 (IPv4)"
LSOv2IPv4 		 = "大型傳送卸載 v2 (IPv4)"
LSOv2IPv6 		 = "大型傳送卸載 v2 (IPv6)"
NetAddress   		 = "網路位址"
WakeUpCapabilities       = "喚醒功能"
APSmode			 = "APS 模式"
AZPower                  = "802.3az"
None		         = "無"
LinkChange	         = "Link Change"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "全部"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; German (Standard)
[Strings.0407]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo-Frame"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
8KBMTU      		 = "8 KB MTU"
9KBMTU      		 = "9 KB MTU"
IntMod 			 = "Interrupt Moderation"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max. IRQ pro Sekunde"
Enabled			 = "Aktiviert"
Disabled		 = "Deaktiviert"
SpeedDuplex		 = "Speed & Duplex"
Auto		  	 = "Autonegotiation"
1GFD                     = "1.0 Gbit/s Vollduplex"
10MHD		  	 = "10 Mbit/s Halbduplex"
10MFD		  	 = "10 Mbit/s Vollduplex"
100MHD			 = "100 Mbit/s Halbduplex"
100MFD			 = "100 Mbit/s Vollduplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Shutdown/Wakeup"
RSS			 = "Empfangsskalierung"
TXEna 			 = "Tx aktiviert"
RXEna 			 = "Rx aktiviert"
TXRXEna 		 = "Tx & Rx aktiviert"
ReceiveBuffers 		 = "Pufferempfang"
TransmitBuffers 	 = "Pufferertragung"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
LSOv2IPv4 		 = "Large Send Offload v2 (IPv4)"
LSOv2IPv6 		 = "Large Send Offload v2 (IPv6)"
NetAddress   		 = "Netzwerkadresse"
WakeUpCapabilities       = "WakeUp-Eigenschaften"
APSmode			 = "APS-Modus"
AZPower                  = "802.3az"
None		         = "Keine"
LinkChange	         = "Link Change"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "Alle"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Trama gigante"
2KBMTU      		 = "MTU de 2KB"
3KBMTU      		 = "MTU de 3KB"
4KBMTU      		 = "MTU de 4KB"
5KBMTU      		 = "MTU de 5KB"
6KBMTU      		 = "MTU de 6KB"
7KBMTU      		 = "MTU de 7KB"
8KBMTU      		 = "MTU de 8KB"
9KBMTU      		 = "MTU de 9KB"
IntMod 			 = "Moderación de interrupciones"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "IRQ máx por segundo"
Enabled			 = "Habilitado"
Disabled		 = "Inhabilitado"
SpeedDuplex		 = "Velocidad y Dúplex"
Auto		  	 = "Negociación automática"
1GFD                     = "Dúplex completo 1.0Gbps"
10MHD		  	 = "Dúplex medio 10Mbps"
10MFD		  	 = "Dúplex completo 10Mbps"
100MHD			 = "Dúplex medio 100Mbps"
100MFD			 = "Dúplex completo 100Mbps"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Reactivar cierre"
RSS			 = "Ajuste de escala en lado de recepción"
TXEna 			 = "Transmisión habilitada"
RXEna 			 = "Recepción habilitada"
TXRXEna 		 = "Transmisión y recepción habilitadas"
ReceiveBuffers 		 = "Recibir búferes"
TransmitBuffers 	 = "Búfers de transmisión"
IPChksumOffv4 		 = "Carga de suma de comprobación IPv4"
TCPChksumOffv4 		 = "Carga de suma de comprobación TCP (IPv4)"
TCPChksumOffv6 		 = "Carga de suma de comprobación TCP (IPv6)"
UDPChksumOffv4 		 = "Carga de suma de comprobación UDP (IPv4)"
UDPChksumOffv6 		 = "Carga de suma de comprobación UDP (IPv6)"
LSOv1IPv4 		 = "Gran carga de envío (IPv4)"
LSOv2IPv4 		 = "Gran carga de envío v2 (IPv4)"
LSOv2IPv6 		 = "Gran carga de envío v2 (IPv6)"
NetAddress   		 = "Dirección de red"
WakeUpCapabilities       = "Capacidades de reactivación"
APSmode			 = "Modo APS"
AZPower                  = "802.3az"
None		         = "Ninguno"
LinkChange	         = "Link Change"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "Todo"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
; French (Standard)
[Strings.040C]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Trame Jumbo"
2KBMTU      		 = "MTU de 2 Ko"
3KBMTU      		 = "MTU de 3 Ko"
4KBMTU      		 = "MTU de 4 Ko"
5KBMTU      		 = "MTU de 5 Ko"
6KBMTU      		 = "MTU de 6 Ko"
7KBMTU      		 = "MTU de 7 Ko"
8KBMTU      		 = "MTU de 8 Ko"
9KBMTU      		 = "MTU de 9 Ko"
IntMod 			 = "Modération de l'interruption"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "IRQ maxi. par seconde"
Enabled			 = "Activée"
Disabled		 = "Désactivée"
SpeedDuplex		 = "Vitesse et Duplex"
Auto		  	 = "Négociation automatique"
1GFD                     = "1.0 Gbits/s Duplex intégral"
10MHD		  	 = "10 Mbits/s Semi-duplex"
10MFD		  	 = "10 Mbits/s Duplex intégral"
100MHD			 = "100 Mbits/s Semi-duplex"
100MFD			 = "100 Mbits/s Duplex intégral"
FlowCtrl		 = "Contrôle de flux"
ShutDW			 = "Sortie de veille à l'arrêt"
RSS			 = "Mise à l'échelle côté réception"
TXEna 			 = "Tx activé"
RXEna 			 = "Rx activé"
TXRXEna 		 = "Tx et rx activés"
ReceiveBuffers 		 = "Mémoires tampon de réception"
TransmitBuffers 	 = "Mémoires tampon de transmission"
IPChksumOffv4 		 = "Déchargement de somme de contrôle IPv4"
TCPChksumOffv4 		 = "Déchargement de somme de contrôle TCP (IPv4)"
TCPChksumOffv6 		 = "Déchargement de somme de contrôle TCP (Ipv6)"
UDPChksumOffv4 		 = "Déchargement de somme de contrôle UDP (IPv4)"
UDPChksumOffv6 		 = "Déchargement de somme de contrôle UDP (Ipv6)"
LSOv1IPv4 		 = "Déchargement d'envoi important (IPv4)"
LSOv2IPv4 		 = "Déchargement d'envoi important v2 (IPv4)"
LSOv2IPv6 		 = "Déchargement d'envoi important v2 (IPv6)"
NetAddress   		 = "Adresse réseau"
WakeUpCapabilities       = "Capacités de mise en éveil"
APSmode			 = "Mode APS"
AZPower                  = "802.3az"
None		         = "Aucun"
LinkChange	         = "Changement de liaison"
MagicPacket	         = "WOL Paquet magique"
PatternMatch	         = "WOL Correspondance au modèle"
MagicPacket_PatternMatch = "MagicPack et PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "Tous"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Italian (Standard)
[Strings.0410]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Frame jumbo"
2KBMTU      		 = "MTU 2 KB"
3KBMTU      		 = "MTU 3 KB"
4KBMTU      		 = "MTU 4 KB"
5KBMTU      		 = "MTU 5 KB"
6KBMTU      		 = "MTU 6 KB"
7KBMTU      		 = "MTU 7 KB"
8KBMTU      		 = "MTU 8 KB"
9KBMTU      		 = "MTU 9 KB"
IntMod 			 = "Regolazione di interrupt (interrupt moderation)"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Numero massimo di IRQ per secondo"
Enabled			 = "Abilitata"
Disabled		 = "Disabilitato"
SpeedDuplex		 = "Velocità e duplex"
Auto		  	 = "Negoziazione automatica"
1GFD                     = "Full Duplex 1.0 Gbps"
10MHD		  	 = "Half Duplex 10 Mbps"
10MFD		  	 = "Full Duplex 10 Mbps"
100MHD			 = "Half Duplex 100 Mbps"
100MFD			 = "Full Duplex 100 Mbps"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Attivazione arresto"
RSS			 = "Receive-Side Scaling"
TXEna 			 = "Tx attivato"
RXEna 			 = "Rx attivato"
TXRXEna 		 = "Abilitato Tx e Rx"
ReceiveBuffers 		 = "Buffer di ricezione"
TransmitBuffers 	 = "Buffer di trasmissione"
IPChksumOffv4 		 = "Offload checksum IPv4"
TCPChksumOffv4 		 = "Offload di checksum TCP (IPv4)"
TCPChksumOffv6 		 = "Offload di checksum TCP (IPv6)"
UDPChksumOffv4 		 = "Offload di checksum UDP (IPv4)"
UDPChksumOffv6 		 = "Offload di checksum UDP (IPv6)"
LSOv1IPv4 		 = "Offload invio di grandi dimensioni (IPv4)"
LSOv2IPv4 		 = "Offload invio di grandi dimensioni v2 (IPv4)"
LSOv2IPv6 		 = "Offload invio di grandi dimensioni v2 (IPv6)"
NetAddress   		 = "Indirizzo di rete"
WakeUpCapabilities       = "Capacità di attivazione"
APSmode			 = "Modalità APS"
AZPower                  = "802.3az"
None		         = "Nessuno"
LinkChange	         = "Modifica collegamento"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Corrispondenza motivo"
MagicPacket_PatternMatch = "MagicPacket e PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "Tutti"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Japanese
[Strings.0411]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "ジャンボ フレーム"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
8KBMTU      		 = "8 KB MTU"
9KBMTU      		 = "9 KB MTU"
IntMod 			 = "割り込み調停"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "最大 IRQ/秒"
Enabled			 = "有効化"
Disabled		 = "無効化"
SpeedDuplex		 = "スピードと二重"
Auto		  	 = "自動ネゴシエーション"
1GFD                     = "1.0 Gbps 全二重"
10MHD		  	 = "10 Mbps 半二重"
10MFD		  	 = "10 Mbps 全二重"
100MHD			 = "100 Mbps 半二重"
100MFD			 = "100 Mbps 全二重"
FlowCtrl		 = "FlowControl"
ShutDW			 = "シャットダウン ウェークアップ"
RSS			 = "受信側スケーリング"
TXEna 			 = "Tx 有効化"
RXEna 			 = "Rx 有効化"
TXRXEna 		 = "Tx と Rx の有効化"
ReceiveBuffers 		 = "受信バッファ"
TransmitBuffers 	 = "送信バッファ"
IPChksumOffv4 		 = "IPv4 チェックサム オフロード"
TCPChksumOffv4 		 = "TCP チェックサム オフロード (IPv4)"
TCPChksumOffv6 		 = "TCP チェックサム オフロード (IPv6)"
UDPChksumOffv4 		 = "UDP チェックサム オフロード (IPv4)"
UDPChksumOffv6 		 = "UDP チェックサム オフロード (IPv6)"
LSOv1IPv4 		 = "大量送信オフロード (IPv4)"
LSOv2IPv4 		 = "大量送信オフロード v2 (IPv4)"
LSOv2IPv6 		 = "大量送信オフロード v2 (IPv6)"
NetAddress   		 = "ネットワーク アドレス"
WakeUpCapabilities       = "ウェークアップ機能"
APSmode			 = "APS モード"
AZPower                  = "802.3az"
None		         = "なし"
LinkChange	         = "リンク変更"
MagicPacket	         = "WOL マジック パケット"
PatternMatch	         = "WOL パターン マッチ"
MagicPacket_PatternMatch = "MagicPacket と PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "すべて"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Dutch (Netherlands)
[Strings.0413]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumboframe"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
8KBMTU      		 = "8 KB MTU"
9KBMTU      		 = "9 KB MTU"
IntMod 			 = "Interruptcontrole"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max. IRQ per seconde"
Enabled			 = "Ingeschakeld"
Disabled		 = "Uitgeschakeld"
SpeedDuplex		 = "Snelheid en duplex"
Auto		  	 = "Automatisch onderhandelen"
1GFD                     = "1.0 Gbps volledige duplex"
10MHD		  	 = "10 Mbps half-duplex"
10MFD		  	 = "10 Mbps volledige duplex"
100MHD			 = "100 Mbps half-duplex"
100MFD			 = "100 Mbps volledige duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Afsluiten Ontwaken"
RSS			 = "Schalen aan de ontvangstzijde"
TXEna 			 = "Tx ingeschakeld"
RXEna 			 = "Rx ingeschakeld"
TXRXEna 		 = "Tx en Rx ingeschakeld"
ReceiveBuffers 		 = "Buffers ontvangen"
TransmitBuffers 	 = "Buffers verzenden"
IPChksumOffv4 		 = "Offload van IPv4-controlesom"
TCPChksumOffv4 		 = "Offload van TCP-controlesom (IPv4)"
TCPChksumOffv6 		 = "Offload van TCP-controlesom (IPv6)"
UDPChksumOffv4 		 = "Offload van UDP-controlesom (IPv4)"
UDPChksumOffv6 		 = "Offload van UDP-controlesom (IPv6)"
LSOv1IPv4 		 = "Grote verzendings-offload (IPv4)"
LSOv2IPv4 		 = "Grote verzendings-offload v2 (IPv4)"
LSOv2IPv6 		 = "Grote verzendings-offload v2 (IPv6)"
NetAddress   		 = "Netwerkadres"
WakeUpCapabilities       = "Mogelijkheden voor ontwaken"
APSmode			 = "APS-modus"
AZPower                  = "802.3az"
None		         = "Geen"
LinkChange	         = "Wijziging koppeling"
MagicPacket	         = "WOL Magic-pakket"
PatternMatch	         = "WOL Patroonovereenkomst"
MagicPacket_PatternMatch = "Magic-pakket en Patroonovereenkomst"
VLanID                   = "VLAN ID"
All 			 = "Alles"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Portuguese (Brazil)
[Strings.0416]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Interromper Moderação"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max IRQ por Segundo"
Enabled			 = "Activado"
Disabled		 = "Desactivado"
SpeedDuplex		 = "Velocidade e Duplex"
Auto		  	 = "Negociação Auotmática"
1GFD                     = "1.0 Gbps Full Duplex"
10MHD		  	 = "10 Mbps Half Duplex"
10MFD		  	 = "10 Mbps Full Duplex"
100MHD			 = "100 Mbps Half Duplex"
100MFD			 = "100 Mbps Full Duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Encerramento Reactivação"
RSS			 = "Receive Side Scaling"
TXEna 			 = "Tx Activada"
RXEna 			 = "Rx Activada"
TXRXEna 		 = "Tx e Rx Activadas"
ReceiveBuffers 		 = "Buffers de Recepção"
TransmitBuffers 	 = "Buffers de Transmissão"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
LSOv2IPv4 		 = "Large Send Offload v2 (IPv4)"
LSOv2IPv6 		 = "Large Send Offload v2 (IPv6)"
NetAddress   		 = "Endereço de Rede"
WakeUpCapabilities       = "Capacidades de Reactivação"
APSmode			 = "Modo APS"
AZPower                  = "802.3az"
None		         = "Nenhum"
LinkChange	         = "Alteração de Ligação"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Correspondência por Padrão"
MagicPacket_PatternMatch = "MagicPacket e Correspondência por Padrão"
VLanID                   = "VLAN ID"
All 			 = "Todos"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Chinese (PRC)
[Strings.0804]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo 帧"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "中断裁决"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "每秒最大 IRQ"
Enabled			 = "启用"
Disabled		 = "禁用"
SpeedDuplex		 = "速度和双工"
Auto		  	 = "自动协商"
1GFD                     = "1.0 Gbps 全双工"
10MHD		  	 = "10 Mbps 半双工"
10MFD		  	 = "10 Mbps 全双工"
100MHD			 = "100 Mbps 半双工"
100MFD			 = "100 Mbps 全双工"
FlowCtrl		 = "流控制"
ShutDW			 = "关闭状态唤醒"
RSS			 = "接收方缩放"
TXEna 			 = "Tx 已启用"
RXEna 			 = "Rx 已启用"
TXRXEna 		 = "Tx 和 Rx 已启用"
ReceiveBuffers 		 = "接收缓冲区"
TransmitBuffers 	 = "传输缓冲区"
IPChksumOffv4 		 = "IPv4 校验和卸载"
TCPChksumOffv4 		 = "TCP 校验和卸载 (IPv4)"
TCPChksumOffv6 		 = "TCP 校验和卸载 (IPv6)"
UDPChksumOffv4 		 = "UDP 校验和卸载 (IPv4)"
UDPChksumOffv6 		 = "UDP 校验和卸载 (IPv6)"
LSOv1IPv4 		 = "大量发送卸载 (IPv4)"
LSOv2IPv4 		 = "大量发送卸载 v2 (IPv4)"
LSOv2IPv6 		 = "大量发送卸载 v2 (IPv6)"
NetAddress   		 = "网络地址"
WakeUpCapabilities       = "唤醒功能"
APSmode			 = "APS 模式"
AZPower                  = "802.3az"
None		         = "无"
LinkChange	         = "链接更改"
MagicPacket	         = "WOL 幻数据包"
PatternMatch	         = "WOL 模式匹配"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "全部"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Czech
[Strings.0405]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Zmírnění přerušení"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Maximální počet IRQ za vteřinu"
Enabled			 = "Zapnuto"
Disabled		 = "Vypnuto"
SpeedDuplex		 = "Rychlost a duplex"
Auto		  	 = "Automatické vyjednávání"
1GFD                     = "Plný duplex 1.0 Gb/s"
10MHD		  	 = "Poloviční duplex 10 Mb/s"
10MFD		  	 = "Plný duplex 10 Mb/s"
100MHD			 = "Poloviční duplex 100 Mb/s"
100MFD			 = "Plný duplex 100 Mb/s"
FlowCtrl		 = "Řízení toku"
ShutDW			 = "Probuzení vypnutého počítače"
RSS			 = "RSS (příchozí procesy mezi více procesorů)"
TXEna 			 = "Tx zapnuto"
RXEna 			 = "Rx zapnuto"
TXRXEna 		 = "Tx a Rx zapnuto"
ReceiveBuffers 		 = "Vyrovnávací paměť příjmu"
TransmitBuffers 	 = "Vyrovnávací paměť odesílání"
IPChksumOffv4 		 = "Odstranění kontrolního součtu u protokolu IPv4"
TCPChksumOffv4 		 = "Odstranění kontrolního součtu u protokolu TCP (IPv4)"
TCPChksumOffv6 		 = "Odstranění kontrolního součtu u protokolu TCP (IPv6)"
UDPChksumOffv4 		 = "Odstranění kontrolního součtu u protokolu UDP (IPv4)"
UDPChksumOffv6 		 = "Odstranění kontrolního součtu u protokolu UDP (IPv6)"
LSOv1IPv4 		 = "Snižování zátěže u rozsáhlého odesílání (IPv4)"
LSOv2IPv4 		 = "Snižování zátěže u rozsáhlého odesílání v2 (IPv4)"
LSOv2IPv6 		 = "Snižování zátěže u rozsáhlého odesílání v2 (IPv6)"
NetAddress   		 = "Adresa sítě"
WakeUpCapabilities       = "Schopnosti probuzení počítače"
APSmode			 = "Režim APS"
AZPower                  = "802.3az"
None		         = "Žádný"
LinkChange	         = "WOL Změna linky"
MagicPacket	         = "WOL Magický paket"
PatternMatch	         = "Porovnávací vzorek"
MagicPacket_PatternMatch = "Magický paket a porovnávací vzorek"
VLanID                   = "VLAN ID"
All 			 = "Vše"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Danish
[Strings.0406]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumboramme"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Interruptindstilling"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Maks. IRQ pr. sekund"
Enabled			 = "Aktiveret"
Disabled		 = "Deaktiveret"
SpeedDuplex		 = "Hastighed og duplex"
Auto		  	 = "Automatisk forhandling"
1GFD                     = "1.0 Gbps fuld duplex"
10MHD		  	 = "10 Mbps halv duplex"
10MFD		  	 = "10 Mbps fuld duplex"
100MHD			 = "100 Mbps halv duplex"
100MFD			 = "100 Mbps fuld duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Lukning/aktivering"
RSS			 = "Modtag sideskalering"
TXEna 			 = "Tx-aktiveret"
RXEna 			 = "Rx-aktiveret"
TXRXEna 		 = "Tx- og Rx-aktiveret"
ReceiveBuffers 		 = "Modtagelsesbuffere"
TransmitBuffers 	 = "Afsendelsesbuffere"
IPChksumOffv4 		 = "Aflastning af IPv4-kontrolsum"
TCPChksumOffv4 		 = "Aflastning af TCP-kontrolsum (IPv4)"
TCPChksumOffv6 		 = "Aflastning af TCP-kontrolsum (IPv6)"
UDPChksumOffv4 		 = "Aflastning af UDP-kontrolsum (IPv4)"
UDPChksumOffv6 		 = "Aflastning af UDP-kontrolsum (IPv6)"
LSOv1IPv4 		 = "Aflastning af for stor forsendelse (IPv4)"
LSOv2IPv4 		 = "Aflastning af for stor forsendelse v2 (IPv4)"
LSOv2IPv6 		 = "Aflastning af for stor forsendelse v2 (IPv6)"
NetAddress   		 = "Netværksadresse"
WakeUpCapabilities       = "Aktiveringsfunktioner"
APSmode			 = "APS-tilstand"
AZPower                  = "802.3az"
None		         = "Ingen"
LinkChange	         = "Forbindelsesændring"
MagicPacket	         = "WOL Magisk pakke"
PatternMatch	         = "WOL Mønstermatch"
MagicPacket_PatternMatch = "Magisk pakke og mønstermatch"
VLanID                   = "VLAN ID"
All 			 = "Alt"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Finnish
[Strings.040b]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo-kehys"
2KBMTU      		 = "2 kt MTU"
3KBMTU      		 = "3 kt MTU"
4KBMTU      		 = "4 kt MTU"
5KBMTU      		 = "5 kt MTU"
6KBMTU      		 = "6 kt MTU"
7KBMTU      		 = "7 kt MTU"
8KBMTU      		 = "8 kt MTU"
9KBMTU      		 = "9 kt MTU"
IntMod 			 = "Keskeytysten lieventäminen"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Enintään IRQ/s"
Enabled			 = "Käytössä"
Disabled		 = "Poissa käytöstä"
SpeedDuplex		 = "Nopeus & kaksisuuntaisuus"
Auto		  	 = "Automaattinen neuvottelu"
1GFD                     = "1.0 Gbps kaksisuuntaisuus"
10MHD		  	 = "10 Mbps vuorosuuntaisuus"
10MFD		  	 = "10 Mbps kaksisuuntaisuus"
100MHD			 = "100 Mbps vuorosuuntaisuus"
100MFD			 = "100 Mbps kaksisuuntaisuus"
FlowCtrl		 = "Vuonohjaus"
ShutDW			 = "Herätys sammutuksesta"
RSS			 = "Vastaanottopuolen skaalaustila"
TXEna 			 = "Tx käytössä"
RXEna 			 = "Rx käytössä"
TXRXEna 		 = "Tx & Rx käytössä"
ReceiveBuffers 		 = "Vastaanottopuskurit"
TransmitBuffers 	 = "Lähetyspuskurit"
IPChksumOffv4 		 = "IPv4-tarkistussumman purku"
TCPChksumOffv4 		 = "TCP-tarkistussumman purku (IPv4)"
TCPChksumOffv6 		 = "TCP-tarkistussumman purku (IPv6)"
UDPChksumOffv4 		 = "UDP-tarkistussumman purku (IPv4)"
UDPChksumOffv6 		 = "UDP-tarkistussumman purku (IPv6)"
LSOv1IPv4 		 = "Suuren lähetyksen purku (IPv4)"
LSOv2IPv4 		 = "Suuren lähetyksen purku v2 (IPv4)"
LSOv2IPv6 		 = "Suuren lähetyksen purku v2 (IPv6)"
NetAddress   		 = "Verkko-osoite"
WakeUpCapabilities       = "Heräämisominaisuudet"
APSmode			 = "Yhteyspistepalvelutila"
AZPower                  = "802.3az"
None		         = "Ei mitään"
LinkChange	         = "Linkin vaihto"
MagicPacket	         = "WOL Magic-paketti"
PatternMatch	         = "WOL Mallivastaavuus"
MagicPacket_PatternMatch = "Magic-paketti & mallivastaavuus"
VLanID                   = "VLAN ID"
All 			 = "Kaikki"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Greek
[Strings.0408]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Πλαίσιο Jumbo"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
8KBMTU      		 = "8 KB MTU"
9KBMTU      		 = "9 KB MTU"
IntMod 			 = "Ρύθμιση διακοπών"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Μέγιστος αριθμός IRQ ανά δευτερόλεπτο"
Enabled			 = "Ενεργοποίηση"
Disabled		 = "Απενεργοποίηση"
SpeedDuplex		 = "Ταχύτητα & αμφίδρομη λειτουργία"
Auto		  	 = "Αυτόματη διαπραγμάτευση"
1GFD                     = "Πλήρως αμφίδρομο 1.0 Gbps"
10MHD		  	 = "Ημι-αμφίδρομο 10 Mbps"
10MFD		  	 = "Πλήρως αμφίδρομο 10 Mbps"
100MHD			 = "Ημι-αμφίδρομο 100 Mbps"
100MFD			 = "Πλήρως αμφίδρομο 100 Mbps"
FlowCtrl		 = "Έλεγχος ροής"
ShutDW			 = "Ενεργοποίηση τερματισμού"
RSS			 = "Καταμερισμός από τον παραλήπτη"
TXEna 			 = "Ενεργοποιημένο Tx"
RXEna 			 = "Ενεργοποιημένο Rx"
TXRXEna 		 = "Ενεργοποιημένο Tx & Rx"
ReceiveBuffers 		 = "Καταχωρητές λήψης"
TransmitBuffers 	 = "Καταχωρητές μετάδοσης"
IPChksumOffv4 		 = "Μείωση φόρτου αθροίσματος ελέγχου IPv4"
TCPChksumOffv4 		 = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv4)"
TCPChksumOffv6 		 = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
UDPChksumOffv4 		 = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv4)"
UDPChksumOffv6 		 = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv6)"
LSOv1IPv4 		 = "Μείωση φόρτου μεγάλης αποστολής (IPv4)"
LSOv2IPv4 		 = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv4)"
LSOv2IPv6 		 = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv6)"
NetAddress   		 = "Διεύθυνση δικτύου"
WakeUpCapabilities       = "Δυνατότητες ενεργοποίησης"
APSmode			 = "Λειτουργία APS"
AZPower                  = "802.3az"
None		         = "Χωρίς"
LinkChange	         = "Αλλαγή σύνδεσης"
MagicPacket	         = "WOL Μαγικό πακέτο"
PatternMatch	         = "WOL Ταίριασμα μοτίβου"
MagicPacket_PatternMatch = "Μαγικό πακέτο & ταίριασμα μοτίβου"
VLanID                   = "VLAN ID"
All 			 = "Όλα"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Hungarian
[Strings.040e]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Óriáskeret"
2KBMTU      		 = "2 kB MTU"
3KBMTU      		 = "3 kB MTU"
4KBMTU      		 = "4 kB MTU"
5KBMTU      		 = "5 kB MTU"
6KBMTU      		 = "6 kB MTU"
7KBMTU      		 = "7 kB MTU"
8KBMTU      		 = "8 kB MTU"
9KBMTU      		 = "9 kB MTU"
IntMod 			 = "Megszakításmérséklés"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Másodpercenkénti maximális IRQ"
Enabled			 = "Engedélyezve"
Disabled		 = "Letiltva"
SpeedDuplex		 = "Sebesség és duplexitás"
Auto		  	 = "Automatikus egyeztetés"
1GFD                     = "1.0 Gbps-os teljes duplex"
10MHD		  	 = "10 Mbps-os fél duplex"
10MFD		  	 = "10 Mbps-os teljes duplex"
100MHD			 = "100 Mbps-os fél duplex"
100MFD			 = "100 Mbps-os teljes duplex"
FlowCtrl		 = "Forgalomszabályozás"
ShutDW			 = "Felébresztés"
RSS			 = "Fogadó oldali méretezés"
TXEna 			 = "Tx engedélyezve"
RXEna 			 = "Rx engedélyezve"
TXRXEna 		 = "Tx és Rx engedélyezve"
ReceiveBuffers 		 = "Fogadási pufferek"
TransmitBuffers 	 = "Átviteli pufferek"
IPChksumOffv4 		 = "IPv4 ellenőrző összeg számításának kihelyezése"
TCPChksumOffv4 		 = "TCP ellenőrző összeg számításának kihelyezése (IPv4)"
TCPChksumOffv6 		 = "TCP ellenőrző összeg számításának kihelyezése (IPv6)"
UDPChksumOffv4 		 = "UDP ellenőrző összeg számításának kihelyezése (IPv4)"
UDPChksumOffv6 		 = "UDP ellenőrző összeg számításának kihelyezése (IPv6)"
LSOv1IPv4 		 = "Tehermentesítés nagy méretű küldés esetén (IPv4)"
LSOv2IPv4 		 = "Tehermentesítés nagy méretű küldés esetén v2 (IPv4)"
LSOv2IPv6 		 = "Tehermentesítés nagy méretű küldés esetén v2 (IPv6)"
NetAddress   		 = "Hálózati cím"
WakeUpCapabilities       = "Ébresztési szolgáltatások"
APSmode			 = "APS mód"
AZPower                  = "802.3az"
None		         = "Nincs"
LinkChange	         = "Csatolásállapot-változás"
MagicPacket	         = "WOL Bűvös csomag"
PatternMatch	         = "WOL Mintaegyezés"
MagicPacket_PatternMatch = "Bűvös csomag és mintaegyezés"
VLanID                   = "VLAN ID"
All 			 = "Összes"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Korean
[Strings.0412]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo 프레임"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "인터럽트 조절"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "초당 최대 IRQ"
Enabled			 = "사용함"
Disabled		 = "사용 안 함"
SpeedDuplex		 = "속도 및 이중성"
Auto		  	 = "자동 협상"
1GFD                     = "1.0 Gbps 전이중"
10MHD		  	 = "10Mbps 반이중"
10MFD		  	 = "10Mbps 전이중"
100MHD			 = "100Mbps 반이중"
100MFD			 = "100Mbps 전이중"
FlowCtrl		 = "흐름 제어(FlowControl)"
ShutDW			 = "중지 모드 해제(Shutdown Wake Up)"
RSS			 = "수신측 배율"
TXEna 			 = "Tx 사용"
RXEna 			 = "Rx 사용"
TXRXEna 		 = "Tx 및 Rx 사용"
ReceiveBuffers 		 = "수신 버퍼"
TransmitBuffers 	 = "전송 버퍼"
IPChksumOffv4 		 = "IPv4 체크섬 오프로드"
TCPChksumOffv4 		 = "TCP 체크섬 오프로드(IPv4)"
TCPChksumOffv6 		 = "TCP 체크섬 오프로드(IPv6)"
UDPChksumOffv4 		 = "UDP 체크섬 오프로드(IPv4)"
UDPChksumOffv6 		 = "UDP 체크섬 오프로드(IPv6)"
LSOv1IPv4 		 = "LSO(Large Send Offload)(IPv4)"
LSOv2IPv4 		 = "LSO(Large Send Offload) v2 (IPv4)"
LSOv2IPv6 		 = "LSO(Large Send Offload) v2 (IPv6)"
NetAddress   		 = "네트워크 주소"
WakeUpCapabilities       = "절전 모드 해제 기능"
APSmode			 = "APS 모드"
AZPower                  = "802.3az"
None		         = "없음"
LinkChange	         = "연결 변경"
MagicPacket	         = "WOL 매직 패킷"
PatternMatch	         = "WOL 패턴 일치"
MagicPacket_PatternMatch = "매직 패킷 및 패턴 일치"
VLanID                   = "VLAN ID"
All 			 = "전체"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Norwegian
[Strings.0414]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2 kB MTU"
3KBMTU      		 = "3 kB MTU"
4KBMTU      		 = "4 kB MTU"
5KBMTU      		 = "5 kB MTU"
6KBMTU      		 = "6 kB MTU"
7KBMTU      		 = "7 kB MTU"
8KBMTU      		 = "8 kB MTU"
9KBMTU      		 = "9 kB MTU"
IntMod 			 = "Avbruddsmoderering"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Maks. IRQ per sekund"
Enabled			 = "Aktivert"
Disabled		 = "Deaktivert"
SpeedDuplex		 = "Hastighet og dupleks"
Auto		  	 = "Autoforhandling"
1GFD                     = "1.0 Gbps full dupleks"
10MHD		  	 = "10 Mbps halv dupleks"
10MFD		  	 = "10 Mbps full dupleks"
100MHD			 = "100 Mbps halv dupleks"
100MFD			 = "100 Mbps full dupleks"
FlowCtrl		 = "Flytkontroll"
ShutDW			 = "Deaktiver oppvåkning"
RSS			 = "Skalering på mottakssiden"
TXEna 			 = "Tx aktivert"
RXEna 			 = "Rx aktivert"
TXRXEna 		 = "Tx og Rx aktivert"
ReceiveBuffers 		 = "Mottaksbuffere"
TransmitBuffers 	 = "Sendebuffere"
IPChksumOffv4 		 = "IPv4-sjekksumavlasting"
TCPChksumOffv4 		 = "TCP-sjekksumavlasting (IPv4)"
TCPChksumOffv6 		 = "TCP-sjekksumavlasting (IPv6)"
UDPChksumOffv4 		 = "UDP-sjekksumavlasting (IPv4)"
UDPChksumOffv6 		 = "UDP-sjekksumavlasting (IPv6)"
LSOv1IPv4 		 = "Avlasting ved stor sending (IPv4)"
LSOv2IPv4 		 = "Avlasting ved stor sending v2 (IPv4)"
LSOv2IPv6 		 = "Avlasting ved stor sending v2 (IPv6)"
NetAddress   		 = "Nettverksadresse"
WakeUpCapabilities       = "Oppvåkingsmuligheter"
APSmode			 = "APS-modus"
AZPower                  = "802.3az"
None		         = "Ingen"
LinkChange	         = "Forbindelsesendring"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Mønstergjenkjenning"
MagicPacket_PatternMatch = "MagicPacket og mønstergjenkjenning"
VLanID                   = "VLAN ID"
All 			 = "Alle"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Polish
[Strings.0415]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Ramka Jumbo"
2KBMTU      		 = "MTU 2 KB"
3KBMTU      		 = "MTU 3 KB"
4KBMTU      		 = "MTU 4 KB"
5KBMTU      		 = "MTU 5 KB"
6KBMTU      		 = "MTU 6 KB"
7KBMTU      		 = "MTU 7 KB"
8KBMTU      		 = "MTU 8 KB"
9KBMTU      		 = "MTU 9 KB"
IntMod 			 = "Moderacja przerwań"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Maks. IRQ na sekundę"
Enabled			 = "Włączone"
Disabled		 = "Wyłączone"
SpeedDuplex		 = "Szybkość i dupleks"
Auto		  	 = "Automatyczna negocjacja"
1GFD                     = "1.0 Gb/s pełny dupleks"
10MHD		  	 = "10 Mb/s, półdupleks"
10MFD		  	 = "10 Mb/s, pełny dupleks"
100MHD			 = "100 Mb/s, półdupleks"
100MFD			 = "100 Mb/s, pełny dupleks"
FlowCtrl		 = "Sterowanie przepływem"
ShutDW			 = "Wyłączanie i budzenie"
RSS			 = "Skalowanie odbioru"
TXEna 			 = "Tx włączone"
RXEna 			 = "Rx włączone"
TXRXEna 		 = "Tx i Rx włączone"
ReceiveBuffers 		 = "Bufory odbioru"
TransmitBuffers 	 = "Bufory transmisji"
IPChksumOffv4 		 = "Odciążanie sumy kontrolnej IPv4"
TCPChksumOffv4 		 = "Odciążanie sumy kontrolnej TCP (IPv4)"
TCPChksumOffv6 		 = "Odciążanie sumy kontrolnej TCP (IPv6)"
UDPChksumOffv4 		 = "Odciążanie sumy kontrolnej UDP (IPv4)"
UDPChksumOffv6 		 = "Odciążanie sumy kontrolnej UDP (IPv6)"
LSOv1IPv4 		 = "Odciążanie dużych transmisji (IPv4)"
LSOv2IPv4 		 = "Odciążanie dużych transmisji v2 (IPv4)"
LSOv2IPv6 		 = "Odciążanie dużych transmisji v2 (IPv6)"
NetAddress   		 = "Adres sieciowy"
WakeUpCapabilities       = "Funkcje budzenia"
APSmode			 = "Tryb APS"
AZPower                  = "802.3az"
None		         = "Brak"
LinkChange	         = "Zmiana łącza"
MagicPacket	         = "WOL Pakiet specjalny"
PatternMatch	         = "WOL Dopasowanie do wzorca"
MagicPacket_PatternMatch = "Pakiet specjalny i dopasowanie do wzorca"
VLanID                   = "VLAN ID"
All 			 = "Wszystko"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Russian
[Strings.0419]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Кадры крупных размеров"
2KBMTU      		 = "2 Кб MTU"
3KBMTU      		 = "3 Кб MTU"
4KBMTU      		 = "4 Кб MTU"
5KBMTU      		 = "5 Кб MTU"
6KBMTU      		 = "6 Кб MTU"
7KBMTU      		 = "7 Кб MTU"
8KBMTU      		 = "8 Кб MTU"
9KBMTU      		 = "9 Кб MTU"
IntMod 			 = "Управление прерываниями"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Макс. IRQ в секунду"
Enabled			 = "Включено"
Disabled		 = "Выключено"
SpeedDuplex		 = "Скорость и режим дуплекса"
Auto		  	 = "Автосогласование"
1GFD                     = "1000 Мбит/с, полный дуплекс"
10MHD		  	 = "10 Мбит/с, полудуплекс"
10MFD		  	 = "10 Мбит/с, полный дуплекс"
100MHD			 = "100 Мбит/с, полудуплекс"
100MFD			 = "100 Мбит/с, полный дуплекс"
FlowCtrl		 = "Управление потоком"
ShutDW			 = "Завершение Пробуждение"
RSS			 = "Масштабирование на стороне приема"
TXEna 			 = "Передача включена"
RXEna 			 = "Прием включен"
TXRXEna 		 = "Передача и прием включены"
ReceiveBuffers 		 = "Буферы приема"
TransmitBuffers 	 = "Буферы передачи"
IPChksumOffv4 		 = "Разгрузка операций контрольной суммы IPv4"
TCPChksumOffv4 		 = "Разгрузка операций контрольной суммы ТСР (IPv4)"
TCPChksumOffv6 		 = "Разгрузка операций контрольной суммы TCP (IPv6)"
UDPChksumOffv4 		 = "Разгрузка операций контрольной суммы UDP (IPv4)"
UDPChksumOffv6 		 = "Разгрузка операций контрольной суммы UDP (IPv6)"
LSOv1IPv4 		 = "Разгрузка операций с отправкой больших пакетов (IPv4)"
LSOv2IPv4 		 = "Разгрузка операций с отправкой больших пакетов v2 (IPv4)"
LSOv2IPv6 		 = "Разгрузка операций с отправкой больших пакетов v2 (IPv6)"
NetAddress   		 = "Сетевой адрес"
WakeUpCapabilities       = "Возможности пробуждения"
APSmode			 = "Режим APS"
AZPower                  = "802.3az"
None		         = "Нет"
LinkChange	         = "Смена связи"
MagicPacket	         = "WOL Пакет Magic"
PatternMatch	         = "WOL Соответствие шаблону"
MagicPacket_PatternMatch = "Пакет Magic и соответствие шаблону"
VLanID                   = "VLAN ID"
All 			 = "Все"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Slovak
[Strings.041b]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Rámec Jumbo"
2KBMTU      		 = "2 kB MTU"
3KBMTU      		 = "3 kB MTU"
4KBMTU      		 = "4 kB MTU"
5KBMTU      		 = "5 kB MTU"
6KBMTU      		 = "6 kB MTU"
7KBMTU      		 = "7 kB MTU"
8KBMTU      		 = "8 kB MTU"
9KBMTU      		 = "9 kB MTU"
IntMod 			 = "Moderovanie prerušenia"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max. počet prerušení IRQ za sekundu"
Enabled			 = "Povolené"
Disabled		 = "Zakázané"
SpeedDuplex		 = "Rýchlosť a duplex"
Auto		  	 = "Automatické vyjednávanie"
1GFD                     = "Úplný duplex 1.0 Gb/s"
10MHD		  	 = "Polovičný duplex 10 Mb/s"
10MFD		  	 = "Úplný duplex 10 Mb/s"
100MHD			 = "Polovičný duplex 100 Mb/s"
100MFD			 = "Úplný duplex 100 Mb/s"
FlowCtrl		 = "Riadenie toku"
ShutDW			 = "Vypnutie/prebudenie"
RSS			 = "Prispôsobenie na strane prijímateľa"
TXEna 			 = "Odosielanie povolené"
RXEna 			 = "Príjem povolený"
TXRXEna 		 = "Príjem a odosielanie povolené"
ReceiveBuffers 		 = "Medzipamäť pre príjem"
TransmitBuffers 	 = "Medzipamäť pre odosielanie"
IPChksumOffv4 		 = "Zníženie záťaže pri kontrolných súčtoch protokolu IPv4"
TCPChksumOffv4 		 = "Zníženie záťaže pri kontrolných súčtoch protokolu TCP (IPv4)"
TCPChksumOffv6 		 = "Zníženie záťaže pri kontrolných súčtoch protokolu TCP (IPv6)"
UDPChksumOffv4 		 = "Zníženie záťaže pri kontrolných súčtoch protokolu UDP (IPv4)"
UDPChksumOffv6 		 = "Zníženie záťaže pri kontrolných súčtoch protokolu UDP (IPv6)"
LSOv1IPv4 		 = "Zníženie záťaže pri odosielaní veľkého množstva údajov (IPv4)"
LSOv2IPv4 		 = "Zníženie záťaže pri odosielaní veľkého množstva údajov v2 (IPv4)"
LSOv2IPv6 		 = "Zníženie záťaže pri odosielaní veľkého množstva údajov v2 (IPv6)"
NetAddress   		 = "Sieťová adresa"
WakeUpCapabilities       = "Možnosti prebudenia"
APSmode			 = "Režim APS"
AZPower                  = "802.3az"
None		         = "Žiadne"
LinkChange	         = "Zmena linky"
MagicPacket	         = "WOL Magický paket"
PatternMatch	         = "WOL Zhoda vzorov"
MagicPacket_PatternMatch = "Magický paket a zhoda vzorov"
VLanID                   = "VLAN ID"
All 			 = "Všetko"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Swedish
[Strings.041d]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumboram"
2KBMTU      		 = "2 kB MTU"
3KBMTU      		 = "3 kB MTU"
4KBMTU      		 = "4 kB MTU"
5KBMTU      		 = "5 kB MTU"
6KBMTU      		 = "6 kB MTU"
7KBMTU      		 = "7 kB MTU"
8KBMTU      		 = "8 kB MTU"
9KBMTU      		 = "9 kB MTU"
IntMod 			 = "Avbrottshantering"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Max IRQ per sekund"
Enabled			 = "Aktiverad"
Disabled		 = "Inaktiverad"
SpeedDuplex		 = "Hastighet och duplex"
Auto		  	 = "Automatisk förhandling"
1GFD                     = "1.0 Gbit/s full duplex"
10MHD		  	 = "10 Mbit/s halv duplex"
10MFD		  	 = "10 Mbit/s full duplex"
100MHD			 = "100 Mbit/s halv duplex"
100MFD			 = "100 Mbit/s full duplex"
FlowCtrl		 = "Flödeskontroll"
ShutDW			 = "Avstängning, väckning"
RSS			 = "Skalning för mottagare"
TXEna 			 = "Tx-aktiverad"
RXEna 			 = "Rx-aktiverad"
TXRXEna 		 = "Tx- och Rx-aktiverad"
ReceiveBuffers 		 = "Mottagningsbuffertar"
TransmitBuffers 	 = "Sändningsbuffertar"
IPChksumOffv4 		 = "IPv4-kontrollsummeavlastning"
TCPChksumOffv4 		 = "TCP-kontrollsummeavlastning (IPv4)"
TCPChksumOffv6 		 = "TCP-kontrollsummeavlastning (IPv6)"
UDPChksumOffv4 		 = "UDP-kontrollsummeavlastning (IPv4)"
UDPChksumOffv6 		 = "UDP-kontrollsummeavlastning (IPv6)"
LSOv1IPv4 		 = "Avlastning för stor sändning (IPv4)"
LSOv2IPv4 		 = "Avlastning för stor sändning v2 (IPv4)"
LSOv2IPv6 		 = "Avlastning för stor sändning v2 (IPv6)"
NetAddress   		 = "Nätverksadress"
WakeUpCapabilities       = "Väckningsfunktioner"
APSmode			 = "APS-läge"
AZPower                  = "802.3az"
None		         = "Inget"
LinkChange	         = "Länkändring"
MagicPacket	         = "WOL Magiskt paket"
PatternMatch	         = "WOL Mönstermatchning"
MagicPacket_PatternMatch = "Magiskt paket och mönstermatchning"
VLanID                   = "VLAN ID"
All 			 = "Allt"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Turkish
[Strings.041f]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Çerçeve"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Kesme Düzenleme"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Maks IRQ/Saniye"
Enabled			 = "Etkin"
Disabled		 = "Devre dışı"
SpeedDuplex		 = "Hız ve Çift Yönlü"
Auto		  	 = "Otomatik Anlaşma"
1GFD                     = "1.0 Gbps Tam Çift Yönlü"
10MHD		  	 = "10 Mbps Yarı Çift Yönlü"
10MFD		  	 = "10 Mbps Tam Çift Yönlü"
100MHD			 = "100 Mbps Yarı Çift Yönlü"
100MFD			 = "100 Mbps Tam Çift Yönlü"
FlowCtrl		 = "Akış Denetimi"
ShutDW			 = "Kapatma Uyandırma"
RSS			 = "Alma Tarafı Ölçeklendirmesi"
TXEna 			 = "Tx Etkin"
RXEna 			 = "Rx Etkin"
TXRXEna 		 = "Tx ve Rx Etkin"
ReceiveBuffers 		 = "Alma Arabellekleri"
TransmitBuffers 	 = "İletim Arabellekleri"
IPChksumOffv4 		 = "IPv4 Sağlama Toplamı Boşaltma"
TCPChksumOffv4 		 = "TCP Sağlama Toplamı Boşaltma (IPv4)"
TCPChksumOffv6 		 = "TCP Sağlama Toplamı Boşaltma (IPv6)"
UDPChksumOffv4 		 = "UDP Sağlama Toplamı Boşaltma (IPv4)"
UDPChksumOffv6 		 = "UDP Sağlama Toplamı Boşaltma (IPv6)"
LSOv1IPv4 		 = "Büyük Gönderme Boşaltması (IPv4)"
LSOv2IPv4 		 = "Büyük Gönderme Boşaltması v2 (IPv4)"
LSOv2IPv6 		 = "Büyük Gönderme Boşaltması v2 (IPv6)"
NetAddress   		 = "Ağ Adresi"
WakeUpCapabilities       = "Uyandırma Yetenekleri"
APSmode			 = "APS modu"
AZPower                  = "802.3az"
None		         = "Hiçbiri"
LinkChange	         = "Bağlantı Değişikliği"
MagicPacket	         = "WOL Sihirli Paket"
PatternMatch	         = "WOL Desen Eşleştirme"
MagicPacket_PatternMatch = "Sihirli Paket ve Desen Eşleştirme"
VLanID                   = "VLAN ID"
All 			 = "Tümü"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Arabic (Saudi Arabia)
[Strings.0401]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "ار الجامبو"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "مقاطعة متوسطة"
L0sL1Threshold           = "بوابة L0sL1"
MaxIrq			 = "الحد الأقصى لـ IRQ في الثانية"
Enabled			 = "ممكن"
Disabled		 = "معطل"
SpeedDuplex		 = "السرعة والإزدواج"
Auto		  	 = "تفاوض تلقائي"
1GFD                     = "1000 ميجابايت في الثانية ازدواج كامل"
10MHD		  	 = "10 ميجابايت في الثانية نصف ازدواج"
10MFD		  	 = "10 ميجابايت في الثانية ازدواج كامل"
100MHD			 = "ميجابايت في الثانية نصف ازدواج 100"
100MFD			 = "100 ميجابايت في الثانية ازدواج كامل"
FlowCtrl		 = "تحكم التدفق"
ShutDW			 = "ايقاظ إيقاف التشغيل"
RSS			 = "مقياس جانب الاستقبال"
TXEna 			 = "Tx ممكن"
RXEna 			 = "Rx ممكن"
TXRXEna 		 = "Tx & Rx ممكن"
ReceiveBuffers 		 = "حواجز الاستلام"
TransmitBuffers 	 = "حواجز الإرسال"
IPChksumOffv4 		 = "تفريغ IPv4 Checksum"
TCPChksumOffv4 		 = "تفريغ TCP Checksum (IPv4)"
TCPChksumOffv6 		 = "تفريغ TCP Checksum (IPv6)"
UDPChksumOffv4 		 = "تفريغ UDP Checksum (IPv4)"
UDPChksumOffv6 		 = "تفريغ UDP Checksum (IPv6)"
LSOv1IPv4 		 = "تفريغ إرسال كبير (IPv4)"
LSOv2IPv4 		 = "تفريغ إرسال كبير الإصدار الثاني (IPv4)"
LSOv2IPv6 		 = "تفريغ إرسال كبير الإصدار الثاني (IPv6)"
NetAddress   		 = "عنوان الشبكة"
WakeUpCapabilities       = "قدرات الايقاظ"
APSmode			 = "وضع APS"
AZPower                  = "802.3az"
None		         = "بلا"
LinkChange	         = "تغيير الارتباط"
MagicPacket	         = "WOL حزمة سحرية"
PatternMatch	         = "WOL توافق النمط"
MagicPacket_PatternMatch = "حزمة سحرية & توافق النمط"
VLanID                   = "VLAN ID"
All 			 = "الكل"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Croatian
[Strings.041a]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo okvir"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Prekinuto suzbijanje"
L0sL1Threshold           = "L0sL1 pristupnik"
MaxIrq			 = "Maks IRQ na sekundu"
Enabled			 = "Aktivirano"
Disabled		 = "Deaktivirano"
SpeedDuplex		 = "Brzina & Dupleks"
Auto		  	 = "Samostalno pregovaranje"
1GFD                     = "1.0 Gbps puni dupleks"
10MHD		  	 = "10 Mbps polu dupleks"
10MFD		  	 = "10 Mbps puni dupleks"
100MHD			 = "100 Mbps polu dupleks"
100MFD			 = "100 Mbps puni dupleks"
FlowCtrl		 = "Nadzor protoka"
ShutDW			 = "Buđenje gašenja"
RSS			 = "Primi bočno preračunavanje"
TXEna 			 = "Tx aktiviran"
RXEna 			 = "Rx aktiviran"
TXRXEna 		 = "Tx & Rx aktivirani"
ReceiveBuffers 		 = "Primi međumemoriju"
TransmitBuffers 	 = "Emitiraj međumemoriju"
IPChksumOffv4 		 = "Iskrcavanje IPv4 zbroja za provjeru "
TCPChksumOffv4 		 = "Iskrcavanje TCP zbroja za provjeru (IPv4)"
TCPChksumOffv6 		 = "Iskrcavanje TCP zbroja za provjeru (IPv6)"
UDPChksumOffv4 		 = "Iskrcavanje UDP zbroja za provjeru (IPv4)"
UDPChksumOffv6 		 = "Iskrcavanje UDP zbroja za provjeru (IPv6)"
LSOv1IPv4 		 = "Iskrcavanje velikog slanja (IPv4)"
LSOv2IPv4 		 = "Iskrcavanje velikog slanja v2 (IPv4)"
LSOv2IPv6 		 = "Iskrcavanje velikog slanja v2 (IPv6)"
NetAddress   		 = "Adresa mreže"
WakeUpCapabilities       = "Mogućnosti buđenja"
APSmode			 = "APS način rada"
AZPower                  = "802.3az"
None		         = "Nijedan"
LinkChange	         = "Promjena veze"
MagicPacket	         = "WOL Čaroban paket"
PatternMatch	         = "WOL Podudaranje s uzorcem"
MagicPacket_PatternMatch = "Čarobanpaket & Podudaranjesuzorcem"
VLanID                   = "VLAN ID"
All 			 = "Svi"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Hebrew
[Strings.040d]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "מסגרת ענקית"
2KBMTU      		 = "2 ק''ב MTU (יחידת שליחה מירבית)"
3KBMTU      		 = "3 ק''ב MTU"
4KBMTU      		 = "4 ק''ב MTU"
5KBMTU      		 = "5 ק''ב MTU"
6KBMTU      		 = "6 ק''ב MTU"
7KBMTU      		 = "7 ק''ב MTU"
8KBMTU      		 = "8 ק''ב MTU"
9KBMTU      		 = "9 ק''ב MTU"
IntMod 			 = "הפרעת המתינות"
L0sL1Threshold           = "מעבר (Gateway) L0sL1"
MaxIrq			 = "IRQ (בקשת הפרעה) מירביות בשניה"
Enabled			 = "פעיל"
Disabled		 = "מנוטרל"
SpeedDuplex		 = "מהירות ודופלקס"
Auto		  	 = "מו''מ אוטומטי"
1GFD                     = "דופלקס מלא 1000 מ''ב/שנייה"
10MHD		  	 = "חצי דופלקס 10 מ''ב/שנייה"
10MFD		  	 = "דופלקס מלא 10 מ''ב/שנייה"
100MHD			 = "חצי דופלקס 100 מ''ב/שנייה"
100MFD			 = "דופלקס מלא 100 מ''ב/שנייה"
FlowCtrl		 = "בקרת תנועה"
ShutDW			 = "התעוררות ממצב כבוי"
RSS			 = "קבל מדידות צדדיות"
TXEna 			 = "הפעל Tx"
RXEna 			 = "הפעל Rx"
TXRXEna 		 = "הפעל Tx ו-Rx"
ReceiveBuffers 		 = "קבל בופרים"
TransmitBuffers 	 = "שדר בופרים"
IPChksumOffv4 		 = "שחרור סיכום ביקורת IPv4"
TCPChksumOffv4 		 = "שחרור סיכום ביקורת TCP (IPv4)"
TCPChksumOffv6 		 = "שחרור סיכום ביקורת TCP (IPv6)"
UDPChksumOffv4 		 = "שחרור סיכום ביקורת UDP (IPv4)"
UDPChksumOffv6 		 = "שחרור סיכום ביקורת UDP (IPv6)"
LSOv1IPv4 		 = "שליחת שחרור גדולה (IPv4)"
LSOv2IPv4 		 = "שליחת שחרור גדולה גירסה 2 (IPv4)"
LSOv2IPv6 		 = "שליחת שחרור גדולה גירסה 2 (IPv6)"
NetAddress   		 = "כתובת רשת"
WakeUpCapabilities       = "יכולות התעוררות"
APSmode			 = "מצב APS"
AZPower                  = "802.3az"
None		         = "ללא"
LinkChange	         = "שינוי חיבור"
MagicPacket	         = "WOL פאקטת קסם (Magic Packet)"
PatternMatch	         = "WOL התאמת תבנית"
MagicPacket_PatternMatch = "התאמת תבנית ופאקטת קסם"
VLanID                   = "VLAN ID"
All 			 = "הכל"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Portuguese (Portugal)
[Strings.0816]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Trama jumbo"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Interromper moderação"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq			 = "Máx. IRQ por segundo"
Enabled			 = "Activado"
Disabled		 = "Desactivado"
SpeedDuplex		 = "Velocidade e duplex"
Auto		  	 = "Negociação auto"
1GFD                     = "1.0 Gbps cheio duplex"
10MHD		  	 = "10 Mbps meio duplex"
10MFD		  	 = "10 Mbps cheio duplex"
100MHD			 = "100 Mbps meio duplex"
100MFD			 = "100 Mbps cheio duplex"
FlowCtrl		 = "Controlo de fluxo"
ShutDW			 = "Fechar despertar"
RSS			 = "Receber escala lateral"
TXEna 			 = "Tx activado"
RXEna 			 = "Rx activado"
TXRXEna 		 = "Tx e Rx activado"
ReceiveBuffers 		 = "Receber memórias intermédias"
TransmitBuffers 	 = "Transmitir memórias intermédias"
IPChksumOffv4 		 = "Descarregar teste por soma IPv4"
TCPChksumOffv4 		 = "Descarregar teste por soma TCP (IPv4)"
TCPChksumOffv6 		 = "Descarregar teste por soma TCP (IPv6)"
UDPChksumOffv4 		 = "Descarregar teste por soma UDP (IPv4)"
UDPChksumOffv6 		 = "Descarregar teste por soma UDP (IPv6)"
LSOv1IPv4 		 = "Descarregar envio grande (IPv4)"
LSOv2IPv4 		 = "Descarregar envio grande v2 (IPv4)"
LSOv2IPv6 		 = "Descarregar envio grande v2 (IPv6)"
NetAddress   		 = "Endereço de rede"
WakeUpCapabilities       = "Capacidades despertar"
APSmode			 = "Modo APS"
AZPower                  = "802.3az"
None		         = "Nenhum"
LinkChange	         = "Alteração de ligação"
MagicPacket	         = "WOL Pacote mágico"
PatternMatch	         = "WOL Combinação padrão"
MagicPacket_PatternMatch = "Pacote mágico e Combinação padrão"
VLanID                   = "VLAN ID"
All 			 = "Todos"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Romanian
[Strings.0418]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Unitate digitală mare de transmitere date"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Moderare Întreruperi"
L0sL1Threshold           = "Portal L0sL1"
MaxIrq			 = "Max IRQ pe secundă"
Enabled			 = "Activat"
Disabled		 = "Dezactivat"
SpeedDuplex		 = "Viteză & Duplex"
Auto		  	 = "Auto Negociere"
1GFD                     = "1.0 Gbps Duplex Complet"
10MHD		  	 = "10 Mbps Semi Duplex"
10MFD		  	 = "10 Mbps Duplex Complet"
100MHD			 = "100 Mbps Semi Duplex"
100MFD			 = "100 Mbps Duplex Complet"
FlowCtrl		 = "Control Transmitere Date"
ShutDW			 = "Oprire Pornire"
RSS			 = "Recepţie Scalare Laterală"
TXEna 			 = "Tx Activat"
RXEna 			 = "Rx Activat"
TXRXEna 		 = "Tx & Rx Activat"
ReceiveBuffers 		 = "Memorii Receptoare"
TransmitBuffers 	 = "Memorii Emiţătoare"
IPChksumOffv4 		 = "Transfer Date IPv4"
TCPChksumOffv4 		 = "Transfer Date TCP (IPv4)"
TCPChksumOffv6 		 = "Transfer Date TCP (IPv6)"
UDPChksumOffv4 		 = "Transfer Date UDP (IPv4)"
UDPChksumOffv6 		 = "Transfer Date UDP (IPv6)"
LSOv1IPv4 		 = "Transfer Mare (IPv4)"
LSOv2IPv4 		 = "Transfer Mare v2 (IPv4)"
LSOv2IPv6 		 = "Transfer Mare v2 (IPv6)"
NetAddress   		 = "Adresă Reţea"
WakeUpCapabilities       = "Capabilităţi Pornire"
APSmode			 = "Mod APS"
AZPower                  = "802.3az"
None		         = "Nimic"
LinkChange	         = "Schimbare Legătură"
MagicPacket	         = "WOL Pachet Magic"
PatternMatch	         = "WOL Potrivire Model"
MagicPacket_PatternMatch = "PachetMagic & PotrivireModel"
VLanID                   = "VLAN ID"
All 			 = "Toate"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Slovenian
[Strings.0424]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Veliki okvir"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "Ublažitev prekinitve"
L0sL1Threshold           = "L0sL1 prehod"
MaxIrq			 = "Maks IRQ na sekundo"
Enabled			 = "Omogočeno"
Disabled		 = "Onemogočeno"
SpeedDuplex		 = "Hitrost in dupleks"
Auto		  	 = "Samodejno pogajanje"
1GFD                     = "1.0 Gbps polni dupleks"
10MHD		  	 = "10 Mbps polovični dupleks"
10MFD		  	 = "10 Mbps polni dupleks"
100MHD			 = "100 Mbps polovični dupleks"
100MFD			 = "100 Mbps polni dupleks"
FlowCtrl		 = "Kontrola pretoka"
ShutDW			 = "Bujenje po izklopu"
RSS			 = "Sprejemno bočno lestvičenje"
TXEna 			 = "Tx omogočeno"
RXEna 			 = "Rx omogočeno"
TXRXEna 		 = "Tx in Rx omogočeno"
ReceiveBuffers 		 = "Sprejemni medpomnilniki"
TransmitBuffers 	 = "Prenosni medpomnilniki"
IPChksumOffv4 		 = "IPv4 kontrolna vsota razbremenitve"
TCPChksumOffv4 		 = "TCP kontrolna vsota razbremenitve (IPv4)"
TCPChksumOffv6 		 = "TCP kontrolna vsota razbremenitve (IPv6)"
UDPChksumOffv4 		 = "UDP kontrolna vsota razbremenitve (IPv4)"
UDPChksumOffv6 		 = "UDP kontrolna vsota razbremenitve (IPv6)"
LSOv1IPv4 		 = "Razbremenitev velikega pošiljanja (IPv4)"
LSOv2IPv4 		 = "Razbremenitev velikega pošiljanja v2 (IPv4)"
LSOv2IPv6 		 = "Razbremenitev velikega pošiljanja v2 (IPv6)"
NetAddress   		 = "Omrežni naslovi"
WakeUpCapabilities       = "Zmožnosti bujenja"
APSmode			 = "APS način"
AZPower                  = "802.3az"
None		         = "Brez"
LinkChange	         = "Sprememba povezave"
MagicPacket	         = "WOL Magični paket"
PatternMatch	         = "WOL Enak vzorec"
MagicPacket_PatternMatch = "Magični paket in Enak vzorec"
VLanID                   = "VLAN ID"
All 			 = "Vse"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."

; Thai
[Strings.041E]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Qualcomm Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
8KBMTU      		 = "8KB MTU"
9KBMTU      		 = "9KB MTU"
IntMod 			 = "ขัดจังหวะการควบคุม"
L0sL1Threshold           = "เกตเวย์ L0sL1"
MaxIrq			 = "IRQ สูงสุดต่ิอวินาที"
Enabled			 = "เปิดใช้งาน"
Disabled		 = "ยกเลิกใช้งาน"
SpeedDuplex		 = "ความเร็ว & ดูเพล็กซ์"
Auto		  	 = "สื่อสารอัตโนมัติ"
1GFD                     = "1.0 Gbps Full Duplex"
10MHD		  	 = "10 Mbps Half Duplex"
10MFD		  	 = "10 Mbps Full Duplex"
100MHD			 = "100 Mbps Half Duplex"
100MFD			 = "100 Mbps Full Duplex"
FlowCtrl		 = "ควบคุมการไหล"
ShutDW			 = "ปิดการปลุก"
RSS			 = "การสเกลด้านรับ"
TXEna 			 = "เปิดใช้งาน Tx"
RXEna 			 = "เปิดใช้งาน Rx"
TXRXEna 		 = "เปิดใช้งาน Tx & Rx"
ReceiveBuffers 		 = "บัฟเฟอร์รับ"
TransmitBuffers 	 = "บัฟเฟอร์ส่ง"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
LSOv2IPv4 		 = "Large Send Offload v2 (IPv4)"
LSOv2IPv6 		 = "Large Send Offload v2 (IPv6)"
NetAddress   		 = "ที่อยู่เครือข่าย"
WakeUpCapabilities       = "ความสามารถปลุก"
APSmode			 = "โหมด APS"
AZPower                  = "802.3az"
None		         = "ไม่มี"
LinkChange	         = "เปลี่ยนลิงก์"
MagicPacket	         = "WOL Magic Packet"
PatternMatch	         = "WOL Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
VLanID                   = "VLAN ID"
All 			 = "ทั้งหมด"
EEE                      = "Energy Efficient Ethernet"
ARPOffload		 = "ARP Offload"
NSOffload		 = "NS Offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

ATHR.L1C 		 = "Atheros AR8131 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L1CD 		 = "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2C 		 = "Atheros AR8132 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1D 		 = "Qualcomm Atheros AR8151 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2CB 		 = "Qualcomm Atheros AR8152/8158 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1F 		 = "Qualcomm Atheros AR8161/8165 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2F 		 = "Qualcomm Atheros AR8162/8166/8168 PCI-E Fast Ethernet Controller (NDIS 6.20)"
ATHR.L1H 		 = "Qualcomm Atheros AR8171/8175 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
ATHR.L2H 		 = "Qualcomm Atheros AR8172/8176/8178 PCI-E Fast Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName 	 = "NDIS Miniport Driver for Qualcomm Atheros AR81xx PCI-E Ethernet Controller"
DriverDisk		 = "Qualcomm Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		 = "This Qualcomm Atheros network Controller connects you to the network."