;
; m4cxwin7
; Supported hardware: D-Link DGE-5xx Gigabit Ethernet Adapter
;
; (C)Copyright 2007-2009 Marvell(R).
; 
; All rights reserved.
;
; inf file for NDIS6.2 Miniport Driver for Windows 7 m4cxwin7.sys

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %D-Link%
CatalogFile	= m4cxwin7.CAT
DriverVer       = 09/28/2009, 11.22.3.3


[Manufacturer]
%D-Link%      = D-Link, NTamd64.6.1, NTx86.6.1,NTamd64.6.0, NTx86.6.0, NTamd64.5.2, NTx86.5.1

[ControlFlags]

ExcludeFromSelect       = *

;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[D-Link]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP / Server 2003
;
;-----------------------------------------------------------------------------
[D-Link.NTx86.5.1]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Server 2003 (64bit)
;
;-----------------------------------------------------------------------------
[D-Link.NTamd64.5.2]
;Empty section


;-----------------------------------------------------------------------------
;
;       Windows Vista
;
;-----------------------------------------------------------------------------
[D-Link.NTamd64.6.0]
;Empty section

[D-Link.NTx86.6.0]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Windows 7
;
;-----------------------------------------------------------------------------
[D-Link.NTamd64.6.1]
;Empty section

[D-Link.NTx86.6.1]
%Yukon-4001.DeviceDesc% = SLYuk2FibGig_CCFE18C6.ndi, PCI\VEN_1186&DEV_4001&SUBSYS_40011186
%Yukon-4B00.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_1186&DEV_4B00&SUBSYS_4B001186
%Yukon-4B01.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1186&DEV_4B01&SUBSYS_4B011186
%Yukon-4B02.DeviceDesc% = SLYuk2FibGig_CCFE18C6.ndi, PCI\VEN_1186&DEV_4B02&SUBSYS_4B021186
%Yukon-4B03.DeviceDesc% = SLYuk2CopGig_7AC15055.ndi, PCI\VEN_1186&DEV_4B03&SUBSYS_4B031186
%Yukon-4C00.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1186&DEV_4C00&SUBSYS_4C001186


;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_18689F27.ndi.NTx86]
DelReg          = m4cxwin7.delreg.Common

AddReg          = m4cxwin7.reg, m4cxwin7.common.params, m4cxwin7.YKVS_SL, m4cxwin7.GigFrSize.params, m4cxwin7.SLSpeedDuplexGig.params, m4cxwin7.SingleLink.params, m4cxwin7.TCPSegm.params, m4cxwin7.TxRxLE.params, m4cxwin7.WoLStd.params, m4cxwin7.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = m4cxwin7.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[SLYuk2CopGig_18689F27.ndi.NTx86.Services]
AddService      = m4cxwin7, 0x02, m4cxwin7.Service, common.EventLog


[SLYuk2CopGig_18689F27.ndi.NTx86.CoInstallers]
AddReg          = m4cxwin7.CoInstallers
CopyFiles       = m4cxwin7.CopyFiles.CoInstallers
;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_7AC15055.ndi.NTx86]
DelReg          = m4cxwin7.delreg.Common

AddReg          = m4cxwin7.reg, m4cxwin7.common.params, m4cxwin7.YKVS_SL, m4cxwin7.GigFrSize.params, m4cxwin7.SLSpeedDuplexGig.params, m4cxwin7.SingleLink.params, m4cxwin7.TxRxLE.params, m4cxwin7.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = m4cxwin7.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[SLYuk2CopGig_7AC15055.ndi.NTx86.Services]
AddService      = m4cxwin7, 0x02, m4cxwin7.Service, common.EventLog


[SLYuk2CopGig_7AC15055.ndi.NTx86.CoInstallers]
AddReg          = m4cxwin7.CoInstallers
CopyFiles       = m4cxwin7.CopyFiles.CoInstallers
;-------------------------------------------------------------------------------
; 

[SLYuk2FibGig_CCFE18C6.ndi.NTx86]
DelReg          = m4cxwin7.delreg.Common

AddReg          = m4cxwin7.reg, m4cxwin7.common.params, m4cxwin7.YKVS_SL, m4cxwin7.GigFrSize.params, m4cxwin7.SingleLink.params, m4cxwin7.TxRxLE.params, m4cxwin7.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = m4cxwin7.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[SLYuk2FibGig_CCFE18C6.ndi.NTx86.Services]
AddService      = m4cxwin7, 0x02, m4cxwin7.Service, common.EventLog


[SLYuk2FibGig_CCFE18C6.ndi.NTx86.CoInstallers]
AddReg          = m4cxwin7.CoInstallers
CopyFiles       = m4cxwin7.CopyFiles.CoInstallers
;-------------------------------------------------------------------------------
; 

[SLYukCopGig_2BA069C3.ndi.NTx86]
DelReg          = m4cxwin7.delreg.Common

AddReg          = m4cxwin7.reg, m4cxwin7.common.params, m4cxwin7.YKVS_SL, m4cxwin7.GigFrSize.params, m4cxwin7.SLSpeedDuplexGig.params, m4cxwin7.SingleLink.params, m4cxwin7.TxRxBuff.params, m4cxwin7.WoLStd.params, m4cxwin7.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = m4cxwin7.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[SLYukCopGig_2BA069C3.ndi.NTx86.Services]
AddService      = m4cxwin7, 0x02, m4cxwin7.Service, common.EventLog


[SLYukCopGig_2BA069C3.ndi.NTx86.CoInstallers]
AddReg          = m4cxwin7.CoInstallers
CopyFiles       = m4cxwin7.CopyFiles.CoInstallers

;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[m4cxwin7.common.params]
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChecksumOffloadIPv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChecksumOffloadIPv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %FixedIntMod%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"

HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %MessageLog%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"


;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[m4cxwin7.TxRxBuff.params]
HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "3"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "500"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "1"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "50"

HKR, Ndi\Params\*TransmitBuffers,ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,Min,		0, "4"
HKR, Ndi\Params\*TransmitBuffers,Max,		0, "200"
HKR, Ndi\Params\*TransmitBuffers,Step,		0, "1"
HKR, Ndi\Params\*TransmitBuffers,Default,	0, "50"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[m4cxwin7.TxRxLE.params]
HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "512"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "256"

HKR, Ndi\Params\*TransmitBuffers,	ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,	Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,	Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,	Min,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Max,		0, "512"
HKR, Ndi\Params\*TransmitBuffers,	Step,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Default,	0, "256"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[m4cxwin7.GigFrSize.params]
HKR, Ndi\params\*JumboPacket,	ParamDesc,	0, %JumboPacket%
HKR, Ndi\params\*JumboPacket,	Type,		0, "enum"
HKR, Ndi\params\*JumboPacket\enum,	"0",	0, "%Bytes1514%"
HKR, Ndi\params\*JumboPacket\enum,	"1",	0, "%Bytes4088%"
HKR, Ndi\params\*JumboPacket\enum,	"2",	0, "%Bytes9014%"
HKR, Ndi\params\*JumboPacket,	Default,	0, "0"
HKR,, *JumboPacket,, "0"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[m4cxwin7.WoLStd.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "27"

[m4cxwin7.DefaultWfSOFF.params]
HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShutdown%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "0"
HKR,, WakeFromShutdownMode,, "17"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[m4cxwin7.TcpSegm.params]
HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LsoV1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[m4cxwin7.SingleLink.params]

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowControl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"
HKR,, *FlowControl,, "3"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"



[m4cxwin7.SLSpeedDuplexGig.params]
HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "5",        0, %1000MFD%

;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[m4cxwin7.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "m4cxwin7"

;-----------------------------------------------------------------------------
;
; Special Registry Entrries
;
;-----------------------------------------------------------------------------
[m4cxwin7.YKVS_SL]

;Key used by notify object
HKR,, YKVS,, "762751"
;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[m4cxwin7.delreg.Common]
HKR, Ndi\Params\MaxFrameSize
HKR, Ndi\Params\HwChecksum
HKR, Ndi\Params\Moderate
HKR, Ndi\Params\MaxReceives
HKR, Ndi\Params\MaxTransmits
HKR, Ndi\Params\BatteryModeLinkDetection
HKR, Ndi\Params\TcpLargeSend
HKR, Ndi\Params\WakeUpModeCap_A
HKR, Ndi\Params\WakeUpModeCap_B
HKR, Ndi\Params\DuplexCapabilities_A
HKR, Ndi\Params\DuplexCapabilities_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\AutoNegotiation_A
HKR, Ndi\Params\AutoNegotiation_B
HKR, Ndi\Params\Role_A
HKR, Ndi\Params\Role_B
HKR, Ndi\Params\Speed_A
HKR, Ndi\Params\Speed_B
HKR, Ndi\Params\TagHeaderSupport_A
HKR, Ndi\Params\TagHeaderSupport_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\ConnectionType_A
HKR, Ndi\Params\ConnectionType_B
HKR, Ndi\Params\*NetworkAddress
HKR, Ndi\Params\*JumboPacket\enum,1514
HKR, Ndi\Params\*JumboPacket\enum,4088
HKR, Ndi\Params\*JumboPacket\enum,9014
HKR, Ndi\Params\*PriorityVLANTag
HKR,, HwChecksum
HKR,, Moderate
HKR,, MaxReceives
HKR,, MaxTransmits
HKR,, BatteryModeLinkDetection
HKR,, TcpLargeSend
HKR,, WakeUpModeCap_A
HKR,, WakeUpModeCap_B
HKR,, DuplexCapabilities_A
HKR,, DuplexCapabilities_B
HKR,, AutoNegotiation_A
HKR,, AutoNegotiation_B
HKR,, Role_A
HKR,, Role_B
HKR,, Speed_A
HKR,, Speed_B
HKR,, TagHeaderSupport_A
HKR,, TagHeaderSupport_B
HKR,, FlowControl_A
HKR,, FlowControl_B
HKR,, ConnectionType_A
HKR,, ConnectionType_B
HKR,, *NetworkAddress
HKR,, *PriorityVLANTag


;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[m4cxwin7.Service]
DisplayName	= %m4cxwin7.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\m4cxwin7.sys
LoadOrderGroup = NDIS


;-----------------------------------------------------------------------------
;
; Coinstaller
;
;-----------------------------------------------------------------------------
[m4cxwin7.CoInstallers]
HKR,,CoInstallers32,0x00010000,"m4x32coinst.dll,CoInstMP"


[m4cxwin7.CopyFiles.CoInstallers]
m4x32coinst.dll,,,0x2

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\m4cxwin7.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
m4cxwin7.sys	= 1,,
m4x32coinst.dll	= 1,,

[m4cxwin7.CopyFiles]
m4cxwin7.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
m4cxwin7.CopyFiles=	12

m4cxwin7.CopyFiles.CoInstallers = 11

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]

D-Link = "D-Link Corporation"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo Packet"
ReceiveBuffers = "Receive Buffers"
TransmitBuffers = "Transmit Buffers"
IPChecksumOffloadIPv4 = "IPv4 Checksum Offload"
TCPChecksumOffloadIPv4 = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadIPv4 = "UDP Checksum Offload (IPv4)"
LsoV1IPv4 = "Large Send Offload (IPv4)"
TXEna = "Tx Enabled"
RXEna = "Rx Enabled"
TXRXEna = "Tx & Rx Enabled"
NetworkAddress   = "Network Address"
WakeUpModeCap   = "Wake-Up Capabilities"
InterruptModeration = "Interrupt Moderation"
FixedIntMod = "Max IRQ per Sec"
MessageLog = "Log Status Messages"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
Autosense = "Auto-Negotiation"
10MHD = "10 Mbps Half Duplex"
10MFD = "10 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
1000MFD = "1000 Mbps Full Duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change"
SpeedDuplex = "Speed & Duplex"
FlowControl = "Flow Control"
WakeFromShutdown = "Wake From Shutdown"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;-----------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"

Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


;-----------------------------------------------------------------------------

; Chinese (Taiwan)
[Strings.0404]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "巨型包"
ReceiveBuffers = "接收緩衝區"
TransmitBuffers = "傳送緩衝區"
IPChecksumOffloadIPv4 = "卸載IPv4校驗和"
TCPChecksumOffloadIPv4 = "卸載TCP校驗和(IPv4)"
UDPChecksumOffloadIPv4 = "卸載UDP校驗和(IPv4)"
LsoV1IPv4 = "大量傳送負載(IPv4)"
TXEna = "啟用Tx"
RXEna = "啟用Rx"
TXRXEna = "啟用Tx和Rx"
NetworkAddress   = "網路位址"
WakeUpModeCap   = "喚醒功能"
InterruptModeration = "中斷模式"
FixedIntMod = "最大 IRQ數量"
MessageLog = "日誌狀態資訊"
On = "開啟"
Off = "關閉"
Enabled = "啟用"
Disabled = "禁用"
Non = "無"
Err = "錯誤"
Wrn = "警告"
Sta = "狀態資訊"
All = "所有資訊"
Autosense = "自動感應"
10MHD = "10Mbps 半雙工"
10MFD = "10Mbps 全雙工"
100MHD = "100Mbps 半雙工"
100MFD = "100Mbps 全雙工"
1000MFD = "1000Mbps 全雙工"
MagicPacket = "Magic Packet喚醒模式"
PatternMatch = "Pattern Match喚醒模式"
MagPackPattMatch = "MP和PM喚醒模式"
LinkChange = "Link Change喚醒模式"
SpeedDuplex = "速度和雙工"
FlowControl = "流控制"
WakeFromShutdown = "從關閉狀態喚醒"
Bytes1514 = "1514 位元組"
Bytes4088 = "4088 位元組"
Bytes9014 = "9014 位元組"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "巨型包"
ReceiveBuffers = "接收缓冲区"
TransmitBuffers = "传送缓冲区"
IPChecksumOffloadIPv4 = "卸载 IPv4 校验和"
TCPChecksumOffloadIPv4 = "卸载 TCP 校验和 (IPv4)"
UDPChecksumOffloadIPv4 = "卸载 UDP 校验和 (IPv4)"
LsoV1IPv4 = "大量传送负载 (IPv4)"
TXEna = "启用 Tx"
RXEna = "启用 Rx"
TXRXEna = "启用Tx 和 Rx"
NetworkAddress   = "网络地址"
WakeUpModeCap   = "唤醒功能"
InterruptModeration = "中断模式"
FixedIntMod = "最大 IRQ数量"
MessageLog = "日志状态信息"
On = "开"
Off = "关"
Enabled = "启用"
Disabled = "禁用"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
1000MFD = "1000Mbps 全双工"
MagicPacket = "Magic Packet唤醒模式"
PatternMatch = "Pattern Match唤醒模式"
MagPackPattMatch = "MP 和 PM 唤醒模式"
LinkChange = "Link Change唤醒模式"
SpeedDuplex = "速度和双工"
FlowControl = "流控制"
WakeFromShutdown = "从关闭中唤醒"
Bytes1514 = "1514 个字节"
Bytes4088 = "4088 个字节"
Bytes9014 = "9014 个字节"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; German (Standard)
[Strings.0407]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo-Paket"
ReceiveBuffers = "Empfangspuffer"
TransmitBuffers = "Sendepuffer"
IPChecksumOffloadIPv4 = "Verlagerung IPv4-Prüfsumme"
TCPChecksumOffloadIPv4 = "Verlagerung TCP-Prüfsumme (IPv4)"
UDPChecksumOffloadIPv4 = "Verlagerung UDP-Prüfsumme (IPv4)"
LsoV1IPv4 = "Übernahme TCP-Segment. (IPv4)"
TXEna = "Tx aktiviert"
RXEna = "Rx aktiviert"
TXRXEna = "Tx & Rx aktiviert"
NetworkAddress   = "Netzwerkadresse"
WakeUpModeCap   = "Wake-up-Funktionen"
InterruptModeration = "Interrupt-Moderation"
FixedIntMod = "Max. IRQ pro Sek."
MessageLog = "Statusmeldungen protokollieren"
On = "Ein"
Off = "Aus"
Enabled = "Aktiviert"
Disabled = "Deaktiviert"
Non = "Keine"
Err = "Fehler"
Wrn = "Warnungen"
Sta = "Statusmeldungen"
All = "Alle Meldungen"
Autosense = "Automatische Erkennung"
10MHD = "10 Mbit/s Halbduplex"
10MFD = "10 Mbit/s Vollduplex"
100MHD = "100 Mbit/s Halbduplex"
100MFD = "100 Mbit/s Vollduplex"
1000MFD = "1000 Mbit/s Vollduplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Änderung des Link-Status"
SpeedDuplex = "Geschwindigkeit und Duplexmodus"
FlowControl = "Datenflusskontrolle"
WakeFromShutdown = "Wake-up aus abgeschaltetem Zust."
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquete Jumbo"
ReceiveBuffers = "Búferes de recepción"
TransmitBuffers = "Búferes de transmisión"
IPChecksumOffloadIPv4 = "Desc. suma comp.IPv4"
TCPChecksumOffloadIPv4 = "Desc. suma comp. TCP (IPv4)"
UDPChecksumOffloadIPv4 = "Desc. suma comp. UDP (IPv4)"
LsoV1IPv4 = "Desc. envío grande (IPv4)"
TXEna = "Tx activado"
RXEna = "Rx activado"
TXRXEna = "Tx y Rx activados"
NetworkAddress   = "Dirección de red"
WakeUpModeCap   = "Capacidades de reactivación"
InterruptModeration = "Moderación de interrupción"
FixedIntMod = "IRQ máx. por seg."
MessageLog = "Mensajes de estado del registro"
On = "Encendido"
Off = "Apagado"
Enabled = "Activado"
Disabled = "Desactivado"
Non = "Ninguna"
Err = "Errores"
Wrn = "Advertencias"
Sta = "Mensajes de estado"
All = "Todos los mensajes"
Autosense = "Orientación automática"
10MHD = "Dúplex media a 10Mbps"
10MFD = "Dúplex completa a 10Mbps"
100MHD = "Dúplex media a 100Mbps"
100MFD = "Dúplex completa a 100Mbps"
1000MFD = "Dúplex completa a 1000Mbps"
MagicPacket = "Paquete mágico"
PatternMatch = "Coincidencia de modelo"
MagPackPattMatch = "Paq. mág. y coinc. mod."
LinkChange = "Cambio de enlace"
SpeedDuplex = "Velocidad y dúplex del enlace"
FlowControl = "Control de flujo"
WakeFromShutdown = "Reactivación desde el cierre"
Bytes1514 = "1514 bytes"
Bytes4088 = "4088 bytes"
Bytes9014 = "9014 bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; French (Standard)
[Strings.040C]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquet géant"
ReceiveBuffers = "Tampons de réception"
TransmitBuffers = "Tampons de transmission"
IPChecksumOffloadIPv4 = "DéchargTotal de contrôle IPv4"
TCPChecksumOffloadIPv4 = "DéchargTotalContr. TCP(IPv4)"
UDPChecksumOffloadIPv4 = "DéchargTotalContr. UDP(IPv4)"
LsoV1IPv4 = "DéchargeEnvoiImportant (IPv4)"
TXEna = "Tx activée"
RXEna = "Rx activée"
TXRXEna = "Tx & Rx activées"
NetworkAddress   = "Adresse réseau"
WakeUpModeCap   = "Capacités de réveil"
InterruptModeration = "Modération de l'interruption"
FixedIntMod = "IRQ max. par seconde"
MessageLog = "Messages d'état du journal"
On = "Actif"
Off = "Inactif"
Enabled = "Activé(e)"
Disabled = "Désactivé(e)"
Non = "Aucun"
Err = "Erreurs"
Wrn = "Avertissements"
Sta = "Messages d'état"
All = "Tous les messages"
Autosense = "Détection automatique"
10MHD = "10 Mbits/s Semi-duplex"
10MFD = "10 Mbits/s Duplex intégral"
100MHD = "100 Mbits/s Semi-duplex"
100MFD = "100 Mbits/s Duplex intégral"
1000MFD = "1000 Mbits/s Duplex intégral"
MagicPacket = "Paquet magique"
PatternMatch = "Correspondance"
MagPackPattMatch = "Paquet magique & Correspondance"
LinkChange = "Changement de liaison"
SpeedDuplex = "Vitesse de liaison et duplex"
FlowControl = "Contrôle de flux"
WakeFromShutdown = "Réveil après arrêt"
Bytes1514 = "1514 octets"
Bytes4088 = "4088 octets"
Bytes9014 = "9014 octets"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Italian (Standard)
[Strings.0410]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacchetto jumbo"
ReceiveBuffers = "Buffer di ricezione"
TransmitBuffers = "Buffer di trasmissione"
IPChecksumOffloadIPv4 = "Checksum Offload IPv4"
TCPChecksumOffloadIPv4 = "Checksum Offload TCP (IPv4)"
UDPChecksumOffloadIPv4 = "Checksum Offload UDP (IPv4)"
LsoV1IPv4 = "Large Send Offload (IPv4)"
TXEna = "Tx abilitato"
RXEna = "Rx abilitato"
TXRXEna = "Tx & Rx abilitati"
NetworkAddress   = "Indirizzo di rete"
WakeUpModeCap   = "Funzioni Wake Up "
InterruptModeration = "Moderazione interrupt"
FixedIntMod = "Max IRQ per sec"
MessageLog = "Messaggi di stato registro"
On = "ON"
Off = "OFF"
Enabled = "Attivato"
Disabled = "Disattivato"
Non = "Nessuno"
Err = "Errori"
Wrn = "Avvertenze"
Sta = "Messaggi di stato"
All = "Tutti i messaggi"
Autosense = "Autoriconoscimento"
10MHD = "10Mbps half duplex"
10MFD = "10Mbps full duplex"
100MHD = "100Mbps half duplex"
100MFD = "100Mbps full duplex"
1000MFD = "1000Mbps full duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Cambio collegamento"
SpeedDuplex = "Velocità di collegamento e duplex"
FlowControl = "Controllo del flusso"
WakeFromShutdown = "Risveglio da shutdown"
Bytes1514 = "1514 byte"
Bytes4088 = "4088 byte"
Bytes9014 = "9014 byte"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Japanese
[Strings.0411]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "ジャンボ パケット"
ReceiveBuffers = "受信バッファ"
TransmitBuffers = "送信バッファ"
IPChecksumOffloadIPv4 = "IPv4チェックサム オフロード"
TCPChecksumOffloadIPv4 = "TCPチェックサム オフロード(IPv4)"
UDPChecksumOffloadIPv4 = "UDPチェックサム オフロード(IPv4)"
LsoV1IPv4 = "大容量送信オフロード (IPv4)"
TXEna = "Tx 有効"
RXEna = "Rx 有効"
TXRXEna = "Tx & Rx 有効"
NetworkAddress   = "ネットワークアドレス"
WakeUpModeCap   = "ウェイク アップ機能"
InterruptModeration = "割り込み節度"
FixedIntMod = "毎秒最大 IRQ"
MessageLog = "ログ ステータス メッセージ"
On = "オン"
Off = "オフ"
Enabled = "オン"
Disabled = "オフ"
Non = "なし"
Err = "エラー"
Wrn = "警告"
Sta = "ステータス メッセージ"
All = "全てのメッセージ"
Autosense = "自動感知"
10MHD = "10Mbps 半二重"
10MFD = "10Mbps 全二重"
100MHD = "100Mbps 半二重"
100MFD = "100Mbps 全二重"
1000MFD = "1000Mbps 全二重"
MagicPacket = "マジック パケット"
PatternMatch = "パターン マッチ"
MagPackPattMatch = "マジック パケットとパターン マッチ"
LinkChange = "リンクの変更"
SpeedDuplex = "リンク速度とデュプレックス"
FlowControl = "フロー制御"
WakeFromShutdown = "シャットダウンからの起動"
Bytes1514 = "1514 バイト"
Bytes4088 = "4088 バイト"
Bytes9014 = "9014 バイト"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Korean
[Strings.0412]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "점보 패킷"
ReceiveBuffers = "수신 버퍼"
TransmitBuffers = "송신 버퍼"
IPChecksumOffloadIPv4 = "IPv4 검사합계 오프로드"
TCPChecksumOffloadIPv4 = "TCP검사합계오프로드(IPv4)"
UDPChecksumOffloadIPv4 = "UDP검사합계오프로드(IPv4)"
LsoV1IPv4 = "대량송신 오프로드(IPv4)"
TXEna = "Tx 사용"
RXEna = "Rx 사용"
TXRXEna = "Tx & Rx 사용"
NetworkAddress   = "네트워크 주소"
WakeUpModeCap   = "시스템 켜기 기능"
InterruptModeration = "인터럽트 완화"
FixedIntMod = "초당 최대 IRQ"
MessageLog = "로그 상태 메시지"
On = "켜기"
Off = "끄기"
Enabled = "활성화됨"
Disabled = "활성 해제됨"
Non = "없음"
Err = "오류"
Wrn = "경고"
Sta = "상태 메시지"
All = "모든 메시지"
Autosense = "자동 감지"
10MHD = "10Mbps 반이중"
10MFD = "10Mbps 전이중"
100MHD = "100Mbps 반이중"
100MFD = "100Mbps 전이중"
1000MFD = "1000Mbps 전이중"
MagicPacket = "매직 패킷"
PatternMatch = "패턴 일치"
MagPackPattMatch = "매직 패킷 및 패턴 일치"
LinkChange = "링크 변경"
SpeedDuplex = "링크 속도 및 이중성"
FlowControl = "흐름 제어"
WakeFromShutdown = "중지 모드 해제"
Bytes1514 = "1514 바이트"
Bytes4088 = "4088 바이트"
Bytes9014 = "9014 바이트"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Polish
[Strings.0415]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pakiet Jumbo"
ReceiveBuffers = "Bufory odbiorcze"
TransmitBuffers = "Bufory nadawcze"
IPChecksumOffloadIPv4 = "IPv4 ob. sumy kon."
TCPChecksumOffloadIPv4 = "Ob. sumy kon. pak. TCP (IPv4)"
UDPChecksumOffloadIPv4 = "Ob. sumy kon. pak. UDP (IPv4)"
LsoV1IPv4 = "Obs. wys. du. il da.(IPv4)"
TXEna = "Bufory nadawcze wł."
RXEna = "Bufory odbiorcze wł."
TXRXEna = "Bufory nad. i odb. wł."
NetworkAddress   = "Adres sieciowy"
WakeUpModeCap   = "Funkcje budzenia"
InterruptModeration = "Moderacja przerwania"
FixedIntMod = "Maks. IRQ na sek."
MessageLog = "Zapisywanie komunikatów o stat."
On = "Włączone"
Off = "Wyłączone"
Enabled = "Włączony"
Disabled = "Wyłączony"
Non = "Żadne"
Err = "Błędy"
Wrn = "Ostrzeżenia"
Sta = "Komunikaty o statusie"
All = "Wszystkie komunikaty"
Autosense = "Automatyczne wykrywanie"
10MHD = "10 Mbps Półdupleks"
10MFD = "10 Mbps Pełen dupleks"
100MHD = "100 Mbps Półdupleks"
100MFD = "100 Mbps Pełen dupleks"
1000MFD = "1000 Mbps Pełen dupleks"
MagicPacket = "Magiczny pakiet"
PatternMatch = "Dopasowanie do wzorca"
MagPackPattMatch = "Mag. pak. i dop. do wzor."
LinkChange = "Zmiana łącza"
SpeedDuplex = "Szybkość i Dupleks"
FlowControl = "Kontrola przepływu danych"
WakeFromShutdown = "Pobudka z zamknięcia"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Portuguese (Brazil)
[Strings.0416]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacote Jumbo"
ReceiveBuffers = "Buffers de Recepção"
TransmitBuffers = "Buffers de Transmissão"
IPChecksumOffloadIPv4 = "Descarga Soma de Verif. IPv4"
TCPChecksumOffloadIPv4 = "Desc. Soma Verif. TCP (IPv4)"
UDPChecksumOffloadIPv4 = "Desc. Soma Verif. UDP (IPv4)"
LsoV1IPv4 = "Grande Desc. Envio (IPv4)"
TXEna = "Tx habilitado"
RXEna = "Rx habilitado"
TXRXEna = "Tx & Rx habilitado"
NetworkAddress   = "Endereço da Rede"
WakeUpModeCap   = "Capacidades de Despertar"
InterruptModeration = "Moderação de Interrupção"
FixedIntMod = "IRQ Máx por Seg"
MessageLog = "Registrar Mensagens de Estado"
On = "Ligado"
Off = "Desligado"
Enabled = "Ativado"
Disabled = "Desativado"
Non = "Nenhum"
Err = "Erros"
Wrn = "Avisos"
Sta = "Mensagens de Estado"
All = "Todas as Mensagens"
Autosense = "Autodetecção"
10MHD = "Semi Dúplex 10Mbps"
10MFD = "Dúplex Completo 10Mbps"
100MHD = "Semi Dúplex 100Mbps"
100MFD = "Dúplex Completo 100Mbps"
1000MFD = "Dúplex Completo 1000Mbps"
MagicPacket = "Pacote Mágico"
PatternMatch = "Padrão Igualado"
MagPackPattMatch = "Pacote Mágico & Padrão Igual."
LinkChange = "Troca de Vínculo"
SpeedDuplex = "Velocidade de Link e Duplex"
FlowControl = "Controle de Fluxo"
WakeFromShutdown = "Despertar do Shutdown"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"


; Russian
[Strings.0419]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Большой пакет"
ReceiveBuffers = "Буферы приема"
TransmitBuffers = "Буферы передачи"
IPChecksumOffloadIPv4 = "Разг.контр.сумм IPv4"
TCPChecksumOffloadIPv4 = "Разг.контр.сумм TCP (IPv4)"
UDPChecksumOffloadIPv4 = "Разг.контр.сумм UDP (IPv4)"
LsoV1IPv4 = "Разг.больш.передач (IPv4)"
TXEna = "Tx включен"
RXEna = "Rx включен"
TXRXEna = "Tx & Rx включен"
NetworkAddress   = "Сетевой адрес"
WakeUpModeCap   = "Возможности пробуждения"
InterruptModeration = "Управление прерываниями"
FixedIntMod = "Макс. IRQ в сек."
MessageLog = "Записывать статус. сообщения"
On = "Вкл."
Off = "Выкл."
Enabled = "Включать" 
Disabled = "Отключать"
Non = "Нет"
Err = "Ошибки"
Wrn = "Предупреждения"
Sta = "Статусные сообщения"
All = "Все сообщения"
Autosense = "Автоопределение"
10MHD = "10Мбит/с полудуплекс"
10MFD = "10Мбит/с полный дуплекс"
100MHD = "100Мбит/с полудуплекс"
100MFD = "100Мбит/с полный дуплекс"
1000MFD = "1000Мбит/с полный дуплекс"
MagicPacket = "Магический пакет"
PatternMatch = "Соответствие схеме"
MagPackPattMatch = "Маг. пакет и Соответствие схеме"
LinkChange = "Измен. статуса соединения"
SpeedDuplex = "Скорость и дуплекс"
FlowControl = "Управление потоком данных"
WakeFromShutdown = "Пробужден. из выключ. состояния"
Bytes1514 = "1514 байт"
Bytes4088 = "4088 байт"
Bytes9014 = "9014 байт"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link DGE-5xx Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter (rev.B)"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter (rev.A)"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxwin7.DriverDesc = "NDIS6.2 Miniport Driver for D-Link DGE-5xx Gigabit Ethernet Adapter"