; This INF file installs the Silicon Image non-Raid driver for the SiI 680
; ATA controller on systems running Windows 2000, Windows XP,
; Windows Server 2003, and Windows Vista.

;
; Copyright (C) 2001-2009 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Windows NT$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
CatalogFile=pnp680.cat
DriverVer=07/28/2009, 1.2.30.1


[SourceDisksNames]
1="Silicon Image ATA/133 Driver Installation Disk",pnp680.sys,,

[SourceDisksFiles]
pnp680.sys	= 1
SilSupp.dll	= 1

[DestinationDirs]
DefaultDestDir		= 12
DllFiles			= 11


[DriverFiles_NT]
PnP680.sys,,,0x20

[DllFiles]
SilSupp.dll,,,0x20


[Manufacturer]
%SI%=SI_HDC

[SI_HDC]
%PCI\VEN_1095&DEV_0680.DeviceDesc%=SI_680, PCI\VEN_1095&DEV_0680&SUBSYS_06801095
%PCI\VEN_1095&DEV_0680.DeviceDesc%=SI_680, PCI\VEN_1095&DEV_0680&SUBSYS_01411028
%PCI\VEN_1095&DEV_0680.DeviceDesc%=SI_680, PCI\VEN_1095&DEV_0680&SUBSYS_901B104D



[SI_680.NTX86]
Copyfiles=DriverFiles_NT, DllFiles

[SI_680.NTX86.Services]
AddService=Pnp680,0x00000002,SI_680_Service_Install, Miniport_EventLog_Inst

[SI_680.NTX86.CoInstallers]
Copyfiles=DllFiles
AddReg = SI_680_CoInstall_AddReg

[SI_680_CoInstall_AddReg]
HKR,,CoInstallers32,0x00010000,"SilSupp.dll, CoInstHandler"

[SI_680_Service_Install]
DisplayName=%SI680IDE.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\pnp680.sys
LoadOrderGroup=Scsi miniport
AddReg=PnPSupport_AddReg
AddReg=PortConfigure_AddReg
AddReg=BusType_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=Supported680SubSystemIds_AddReg


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


[PortConfigure_AddReg]
HKR,Parameters\Device,NumberOfRequests,0x00010001, 64
HKR,Parameters\Device,MaximumSGList,0x00010001, 33
HKR, Parameters\Device, CreateInitiatorLU, 0x00010001, 1


; Set controller's bus type to ATA.
[BusType_AddReg]
HKR, Parameters, BusType, 0x00010001, 3


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices


; List of controller subsystem IDs to be supported by the PnP680.sys driver.
[Supported680SubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_0680.DeviceDesc%,0x00010001, 0x06801095
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_0680.DeviceDesc% (Dell)",0x00010001, 0x01411028
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_0680.DeviceDesc% (Sony2)",0x00010001, 0x901B104D



;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_0680.DeviceDesc="Silicon Image SiI 0680 ATA/133 Controller"
SI680IDE.SvcDesc="SiI 680 ATA Controller"


