Windows Registry Editor Version 5.00

; This INI file contains the information about registry keys' name, type and data
; that are used by UAA/WDM drivers as Driver Capabilitys when driver is loaded.
; The format of each registry key is defined as following
;  
;     [Key Name]=[Key Type]$[Key Data] 
; 
; Reserved words "[Reg Key Name]", "=" and "$" are basic format and can't be changed. 
; [Key Name] : Registry Name is a string.
; [Key Type] : Registry Key Types used are REG_DWORD(4) and REG_BINARY(3). 
; [Key Data] : Registry Data MUST be a HEXIDECIMAL value.
; Hexidecimal Data
; Asus VT1708S 3 Jack + header support 7.1 of IMBMQ67
; HDAUDIO\FUNC_01&VEN_1106&SUBSYS_10438417
; DCDEF11.Ini

; Base INF Last Updated 6.0.10.1100
; Modify by Sky123.Org (Trangquil)
; Time: 10/23/2012

[RegKey]
; 3 Jack support 7.1 
"DrvAzCom3JacksAs71"=hex:01,00,00,00

; PCbeep 
"PCBeepInExist"=hex:00,00,00,00

"DrvHPAlwaysEnableForVT3310"=hex:01,00,00,00
"DrvFrontMIcDisableExceptCapture"=hex:01,00,00,00
"DrvWidgetsPowerDownAtUnload"=hex:00,00,00,00
"DrvAzComPowerSequence"=hex:01,00,00,00
"DrvAzComMicMode"=hex:02,00,00,00
"DrvAzComUseHDFrontPanel"=hex:01,00,00,00
"DrvMuteAAPathJacksUnPlugged"=hex:00,00,00,00
"DrvAzComMuteHPIfNoJackPlugIn"=hex:01,00,00,00
"DrvAzComSetDefaultCommands"=hex:01,00,00,00

; HDMI
"DrvSPDIFUseAsHDMI"=hex:01,00,00,00
"DrvSPDIFHDMISwitchSupport"=hex:01,00,00,00
"DrvSPDIFTX2Support"=hex:00,00,00,00
"DrvSPDIFHDMI2SwitchSupport"=hex:00,00,00,00

"SpdifInExist"=hex:00,00,00,00

; Setting Recording Max value
"DrvSetRecCDInMaxLvlByIni"=hex:01,00,00,00
"DrvRecCDInMaxLevel"=dword:00140000
"DrvSetRecStereoMixerMaxLvlByIni"=hex:01,00,00,00
"DrvRecStereoMixerMaxLevel"=dword:00030000
"DrvSetRecLineInMaxLvlByIni"=hex:01,00,00,00
"DrvRecLineInMaxLevel"=dword:00140000
"DrvSetRecMicrophoneMaxLvlByIni"=hex:01,00,00,00
"DrvRecMicrophoneMaxLevel"=dword:00140000

[HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\VIA HD Audio Codec Default\DriverCaps]
; 3 Jack support 7.1 
"DrvAzCom3JacksAs71"=hex:01,00,00,00

; PCbeep 
"PCBeepInExist"=hex:00,00,00,00

"DrvHPAlwaysEnableForVT3310"=hex:01,00,00,00
"DrvFrontMIcDisableExceptCapture"=hex:01,00,00,00
"DrvWidgetsPowerDownAtUnload"=hex:00,00,00,00
"DrvAzComPowerSequence"=hex:01,00,00,00
"DrvAzComMicMode"=hex:02,00,00,00
"DrvAzComUseHDFrontPanel"=hex:01,00,00,00
"DrvMuteAAPathJacksUnPlugged"=hex:00,00,00,00
"DrvAzComMuteHPIfNoJackPlugIn"=hex:01,00,00,00
"DrvAzComSetDefaultCommands"=hex:01,00,00,00

; HDMI
"DrvSPDIFUseAsHDMI"=hex:01,00,00,00
"DrvSPDIFHDMISwitchSupport"=hex:01,00,00,00
"DrvSPDIFTX2Support"=hex:00,00,00,00
"DrvSPDIFHDMI2SwitchSupport"=hex:00,00,00,00

"SpdifInExist"=hex:00,00,00,00

; Setting Recording Max value
"DrvSetRecCDInMaxLvlByIni"=hex:01,00,00,00
"DrvRecCDInMaxLevel"=dword:00140000
"DrvSetRecStereoMixerMaxLvlByIni"=hex:01,00,00,00
"DrvRecStereoMixerMaxLevel"=dword:00030000
"DrvSetRecLineInMaxLvlByIni"=hex:01,00,00,00
"DrvRecLineInMaxLevel"=dword:00140000
"DrvSetRecMicrophoneMaxLvlByIni"=hex:01,00,00,00
"DrvRecMicrophoneMaxLevel"=dword:00140000